Back to Release page
# Release Notes for STM32F042K6-Nucleo Examples Copyright 2016 STMicroelectronics
## Update History ### V1.11.0 / 12-September-2019 Main Changes Update HAL CRC examples Remove unwanted default polynomial attribute configuration as there is no programmable polynomial feature Update HAL SPI_FullDuplex_ComDMA example - Update HAL_SPI_MspInit() API to use DMA handle for reception instead of transmission in reception process Update stm32f0xx_hal_conf.h files : Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Add reference to HAL EXTI driver Add registers callbacks defines ### V1.9.0 / 25-August-2017 Main Changes Maintenance release. Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Align stm32f0xx_hal_conf.h with latest template defined in HAL. Change assert_failed() prototype to be compliant with MISRA C rule 11.4 ### V1.8.0 / 07-April-2017 Main Changes Maintenance release Update stm32f0xx_hal_conf.h files : Compliance with MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). Add definition of USE_SPI_CRC ### V1.7.0 / 04-November-2016 Main Changes Maintenance release. Updated WWDG examples to be in line with latest updates done on HAL WWDG drivers Remove the HAL_WWDG_Start and update the HAL_WWDG_Refresh functions in the main.c file Remove HAL_WWDG_MspDeInit function from stm32f4xx_hal_msp.c file Change of HAL API for IWDG : Removal of HAL_IWDG_Start function in the main.c of IWDG example. Updated SPI examples to fix a problem relative to configuration of SPI PIN ### V1.6.0 / 27-May-2016 Main Changes Maintenance release. Updated system_stm32f0xx.c files: Added APBPrescTable definition. ### V1.5.0 / 29-January-2016 Main Changes Maintenance release. Add support of System Workbench for STM32 (SW4STM32) toolchain. Extended set of examples (ADC, CRC, DMA, FLASH, I2C, IWDG, PWR, RTC, SPI, TIM, UART, WWDG) is provided to start new development on STM32F042K6-Nucleo board. Updated GPIO Output Speed literals naming to ensure HAL full compatibility. Updated system_stm32f0xx.c files: Removed __IO or __I on constant table declaration. Added HSI48_VALUE definition. Updated stm32f0xx_hal_conf.h files: Set HSE_STARTUP_TIMEOUT value to 100ms instead of 5000ms Updated “Liberty” License with the new license “Ultimate Liberty”. ### V1.4.0 / 11-September-2015 Main Changes Basic example (GPIO_IOToggle) is provided to easily start new development on STM32F042K6-Nucleo boards. ## License This software component is licensed by ST under BSD 3-Clause license, the "License"; You may not use this component except in compliance with the License. You may obtain a copy of the License at: https://opensource.org/licenses/BSD-3-Clause For complete documentation on STM32 Microcontrollers visit www.st.com/STM32