CMSIS-DAP: Revision History of CMSIS-DAP

| CMSIS-DAP Version 2.0.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Revision History of CMSIS-DAP

Version | Description
--- | ---
V2.0.0 | Changed: Communication via WinUSB to achieve high-speed transfer rates Added: Streaming SWO via separate WinUSB endpoint Added: DAP_SWO_Transport extended with transport mode 2 - Send trace data via separate WinUSB endpoint
V1.2.0 | Added: DAP_SWD_Sequence to enable SWD multi-drop target selection Added: Test Domain Timer values in the commands DAP_Info, DAP_Transfer
V1.1.0 | Added: SWO Commands to support Serial Wire Output (SWO) in UART mode Added: Atomic Commands support for executing time critical DAP commands
V1.0.0 | Version 1.0.0 was never released; version number skipped.
V0.02 | Renamed DAP_LED to DAP_HostStatus.
V0.01 | Beta Release.