CMSIS-Core (Cortex-M): Define values

| CMSIS-Core (Cortex-M) Version 5.1.2 CMSIS-Core support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Macros
Define values
MPU Functions for Armv7-M

Define values for MPU region setup. More...

## Macros
#define | ARM_MPU_REGION_SIZE_xxx
| Size values of a MPU region (in RASR field) More...
#define | ARM_MPU_AP_xxx
| Values for MPU region access permissions (in RASR field) More...
#define | ARM_MPU_ACCESS_xxx
| Values for MPU region access attributes (in RASR field) More...
#define | ARM_MPU_CACHEP_xxx
| Cache policy values for MPU region access attributes (in RASR field) More...

## Description

The following define values are used with ARM_MPU_RASR to setup the RASR value field in the MPU region.

See Also
  ARM_MPU_Region_t, ARM_MPU_SetRegion, ARM_MPU_SetRegionEx.

## Macro Definition Documentation

#define ARM_MPU_ACCESS_xxx

The following define values are used to compose the access attributes for an MPU region:

#define | TEX | Shareable | Cacheable | Bufferable | Description
--- | --- | --- | --- | --- | ---
ARM_MPU_ACCESS_ORDERED | 000b | 1 | 0 | 0 | Strongly ordered memory
ARM_MPU_ACCESS_DEVICE(S) | 0s0b | S | 0 | S | Memory mapped peripheral device, shared (S=1) or non-shared (S=0)
ARM_MPU_ACCESS_NORMAL(O,I,S) | 1BBb | S | A | A | Normal memory, with outer/inner cache policy (O/I=ARM_MPU_CACHEP_xxx, shared (S=1) or non-share (S=0)

#define ARM_MPU_AP_xxx

The following define values are used to compose the access permission for an MPU region:

#define | Value | Access permissions
--- | --- | ---
ARM_MPU_AP_NONE | 0x0U | None: any access generates a permission fault.
ARM_MPU_AP_PRIV | 0x1U | Privileged Read/Write: privileged access only; any unprivileged access generates a permission fault.
ARM_MPU_AP_URO | 0x2U | Privileged Read/Write; Unprivileged Read-only: any unprivileged write generates a permission fault.
ARM_MPU_AP_FULL | 0x3U | Privileged Read/Write. Unprivileged Read/Write: full access, permission faults are never generated.
ARM_MPU_AP_PRO | 0x5U | Privileged Read-only: any unprivileged access or privileged write generates a permission fault.
ARM_MPU_AP_RO | 0x6U | Privileged and Unprivileged Read-only: any write generates a permission fault.

#define ARM_MPU_CACHEP_xxx

The following define values are used to compose the cacheability flags within the access attributes for an MPU region:

#define | Value | Cacheability policy
--- | --- | ---
ARM_MPU_CACHEP_NOCACHE | 00b | Non-cacheable
ARM_MPU_CACHEP_WB_WRA | 01b | Write-back, write and read allocate
ARM_MPU_CACHEP_WT_NWA | 10b | Write-through, no write allocate
ARM_MPU_CACHEP_WB_NWA | 11b | Write-back, no write allocate

#define ARM_MPU_REGION_SIZE_xxx

The following define values are used to compose the size information for an MPU region:

#define | Value | Description
--- | --- | ---
ARM_MPU_REGION_SIZE_32B | 0x04U | Region size 32 Bytes
ARM_MPU_REGION_SIZE_64B | 0x05U | Region size 64 Bytes
ARM_MPU_REGION_SIZE_128B | 0x06U | Region size 128 Bytes
ARM_MPU_REGION_SIZE_256B | 0x07U | Region size 256 Bytes
ARM_MPU_REGION_SIZE_512B | 0x08U | Region size 512 Bytes
ARM_MPU_REGION_SIZE_1KB | 0x09U | Region size 1 KByte
ARM_MPU_REGION_SIZE_2KB | 0x0AU | Region size 2 KBytes
ARM_MPU_REGION_SIZE_4KB | 0x0BU | Region size 4 KBytes
ARM_MPU_REGION_SIZE_8KB | 0x0CU | Region size 8 KBytes
ARM_MPU_REGION_SIZE_16KB | 0x0DU | Region size 16 KBytes
ARM_MPU_REGION_SIZE_32KB | 0x0EU | Region size 32 KBytes
ARM_MPU_REGION_SIZE_64KB | 0x0FU | Region size 64 KBytes
ARM_MPU_REGION_SIZE_128KB | 0x10U | Region size 128 KBytes
ARM_MPU_REGION_SIZE_256KB | 0x11U | Region size 256 KBytes
ARM_MPU_REGION_SIZE_512KB | 0x12U | Region size 512 KBytes
ARM_MPU_REGION_SIZE_1MB | 0x13U | Region size 1 MByte
ARM_MPU_REGION_SIZE_2MB | 0x14U | Region size 2 MBytes
ARM_MPU_REGION_SIZE_4MB | 0x15U | Region size 4 MBytes
ARM_MPU_REGION_SIZE_8MB | 0x16U | Region size 8 MBytes
ARM_MPU_REGION_SIZE_16MB | 0x17U | Region size 16 MBytes
ARM_MPU_REGION_SIZE_32MB | 0x18U | Region size 32 MBytes
ARM_MPU_REGION_SIZE_64MB | 0x19U | Region size 64 MBytes
ARM_MPU_REGION_SIZE_128MB | 0x1AU | Region size 128 MBytes
ARM_MPU_REGION_SIZE_256MB | 0x1BU | Region size 256 MBytes
ARM_MPU_REGION_SIZE_512MB | 0x1CU | Region size 512 MBytes
ARM_MPU_REGION_SIZE_1GB | 0x1DU | Region size 1 GByte
ARM_MPU_REGION_SIZE_2GB | 0x1EU | Region size 2 GBytes
ARM_MPU_REGION_SIZE_4GB | 0x1FU | Region size 4 GBytes