CMSIS-Driver: Globals

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

- All
- Functions
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- c
- d
- e
- f
- i
- m
- n
- p
- r
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - u -

- ARM_USART_ABORT_RECEIVE : Driver_USART.h
- ARM_USART_ABORT_SEND : Driver_USART.h
- ARM_USART_ABORT_TRANSFER : Driver_USART.h
- ARM_USART_API_VERSION : Driver_USART.h
- ARM_USART_Control() : Driver_USART.c
- ARM_USART_CONTROL_BREAK : Driver_USART.h
- ARM_USART_CONTROL_Msk : Driver_USART.h
- ARM_USART_CONTROL_Pos : Driver_USART.h
- ARM_USART_CONTROL_RX : Driver_USART.h
- ARM_USART_CONTROL_SMART_CARD_NACK : Driver_USART.h
- ARM_USART_CONTROL_TX : Driver_USART.h
- ARM_USART_CPHA0 : Driver_USART.h
- ARM_USART_CPHA1 : Driver_USART.h
- ARM_USART_CPHA_Msk : Driver_USART.h
- ARM_USART_CPHA_Pos : Driver_USART.h
- ARM_USART_CPOL0 : Driver_USART.h
- ARM_USART_CPOL1 : Driver_USART.h
- ARM_USART_CPOL_Msk : Driver_USART.h
- ARM_USART_CPOL_Pos : Driver_USART.h
- ARM_USART_DATA_BITS_5 : Driver_USART.h
- ARM_USART_DATA_BITS_6 : Driver_USART.h
- ARM_USART_DATA_BITS_7 : Driver_USART.h
- ARM_USART_DATA_BITS_8 : Driver_USART.h
- ARM_USART_DATA_BITS_9 : Driver_USART.h
- ARM_USART_DATA_BITS_Msk : Driver_USART.h
- ARM_USART_DATA_BITS_Pos : Driver_USART.h
- ARM_USART_DTR_CLEAR : Driver_USART.h
- ARM_USART_DTR_SET : Driver_USART.h
- ARM_USART_ERROR_BAUDRATE : Driver_USART.h
- ARM_USART_ERROR_CPHA : Driver_USART.h
- ARM_USART_ERROR_CPOL : Driver_USART.h
- ARM_USART_ERROR_DATA_BITS : Driver_USART.h
- ARM_USART_ERROR_FLOW_CONTROL : Driver_USART.h
- ARM_USART_ERROR_MODE : Driver_USART.h
- ARM_USART_ERROR_PARITY : Driver_USART.h
- ARM_USART_ERROR_STOP_BITS : Driver_USART.h
- ARM_USART_EVENT_CTS : Driver_USART.h
- ARM_USART_EVENT_DCD : Driver_USART.h
- ARM_USART_EVENT_DSR : Driver_USART.h
- ARM_USART_EVENT_RECEIVE_COMPLETE : Driver_USART.h
- ARM_USART_EVENT_RI : Driver_USART.h
- ARM_USART_EVENT_RX_BREAK : Driver_USART.h
- ARM_USART_EVENT_RX_FRAMING_ERROR : Driver_USART.h
- ARM_USART_EVENT_RX_OVERFLOW : Driver_USART.h
- ARM_USART_EVENT_RX_PARITY_ERROR : Driver_USART.h
- ARM_USART_EVENT_RX_TIMEOUT : Driver_USART.h
- ARM_USART_EVENT_SEND_COMPLETE : Driver_USART.h
- ARM_USART_EVENT_TRANSFER_COMPLETE : Driver_USART.h
- ARM_USART_EVENT_TX_COMPLETE : Driver_USART.h
- ARM_USART_EVENT_TX_UNDERFLOW : Driver_USART.h
- ARM_USART_FLOW_CONTROL_CTS : Driver_USART.h
- ARM_USART_FLOW_CONTROL_Msk : Driver_USART.h
- ARM_USART_FLOW_CONTROL_NONE : Driver_USART.h
- ARM_USART_FLOW_CONTROL_Pos : Driver_USART.h
- ARM_USART_FLOW_CONTROL_RTS : Driver_USART.h
- ARM_USART_FLOW_CONTROL_RTS_CTS : Driver_USART.h
- ARM_USART_GetCapabilities() : Driver_USART.c
- ARM_USART_GetModemStatus() : Driver_USART.c
- ARM_USART_GetRxCount() : Driver_USART.c
- ARM_USART_GetStatus() : Driver_USART.c
- ARM_USART_GetTxCount() : Driver_USART.c
- ARM_USART_GetVersion() : Driver_USART.c
- ARM_USART_Initialize() : Driver_USART.c
- ARM_USART_MODE_ASYNCHRONOUS : Driver_USART.h
- ARM_USART_MODE_IRDA : Driver_USART.h
- ARM_USART_MODE_SINGLE_WIRE : Driver_USART.h
- ARM_USART_MODE_SMART_CARD : Driver_USART.h
- ARM_USART_MODE_SYNCHRONOUS_MASTER : Driver_USART.h
- ARM_USART_MODE_SYNCHRONOUS_SLAVE : Driver_USART.h
- ARM_USART_MODEM_CONTROL : Driver_USART.h
- ARM_USART_PARITY_EVEN : Driver_USART.h
- ARM_USART_PARITY_Msk : Driver_USART.h
- ARM_USART_PARITY_NONE : Driver_USART.h
- ARM_USART_PARITY_ODD : Driver_USART.h
- ARM_USART_PARITY_Pos : Driver_USART.h
- ARM_USART_PowerControl() : Driver_USART.c
- ARM_USART_Receive() : Driver_USART.c
- ARM_USART_RTS_CLEAR : Driver_USART.h
- ARM_USART_RTS_SET : Driver_USART.h
- ARM_USART_Send() : Driver_USART.c
- ARM_USART_SET_DEFAULT_TX_VALUE : Driver_USART.h
- ARM_USART_SET_IRDA_PULSE : Driver_USART.h
- ARM_USART_SET_SMART_CARD_CLOCK : Driver_USART.h
- ARM_USART_SET_SMART_CARD_GUARD_TIME : Driver_USART.h
- ARM_USART_SetModemControl() : Driver_USART.c
- ARM_USART_SignalEvent() : Driver_USART.c
- ARM_USART_SignalEvent_t : Driver_USART.h
- ARM_USART_STOP_BITS_0_5 : Driver_USART.h
- ARM_USART_STOP_BITS_1 : Driver_USART.h
- ARM_USART_STOP_BITS_1_5 : Driver_USART.h
- ARM_USART_STOP_BITS_2 : Driver_USART.h
- ARM_USART_STOP_BITS_Msk : Driver_USART.h
- ARM_USART_STOP_BITS_Pos : Driver_USART.h
- ARM_USART_Transfer() : Driver_USART.c
- ARM_USART_Uninitialize() : Driver_USART.c
- ARM_USB_ENDPOINT_BULK : Driver_USB.h
- ARM_USB_ENDPOINT_CONTROL : Driver_USB.h
- ARM_USB_ENDPOINT_DIRECTION_MASK : Driver_USB.h
- ARM_USB_ENDPOINT_INTERRUPT : Driver_USB.h
- ARM_USB_ENDPOINT_ISOCHRONOUS : Driver_USB.h
- ARM_USB_ENDPOINT_MAX_PACKET_SIZE_MASK : Driver_USB.h
- ARM_USB_ENDPOINT_MICROFRAME_TRANSACTIONS_1 : Driver_USB.h
- ARM_USB_ENDPOINT_MICROFRAME_TRANSACTIONS_2 : Driver_USB.h
- ARM_USB_ENDPOINT_MICROFRAME_TRANSACTIONS_3 : Driver_USB.h
- ARM_USB_ENDPOINT_MICROFRAME_TRANSACTIONS_MASK : Driver_USB.h
- ARM_USB_ENDPOINT_NUMBER_MASK : Driver_USB.h
- ARM_USB_PID_ACK : Driver_USB.h
- ARM_USB_PID_DATA0 : Driver_USB.h
- ARM_USB_PID_DATA1 : Driver_USB.h
- ARM_USB_PID_DATA2 : Driver_USB.h
- ARM_USB_PID_ERR : Driver_USB.h
- ARM_USB_PID_IN : Driver_USB.h
- ARM_USB_PID_MDATA : Driver_USB.h
- ARM_USB_PID_NAK : Driver_USB.h
- ARM_USB_PID_NYET : Driver_USB.h
- ARM_USB_PID_OUT : Driver_USB.h
- ARM_USB_PID_PING : Driver_USB.h
- ARM_USB_PID_PRE : Driver_USB.h
- ARM_USB_PID_RESERVED : Driver_USB.h
- ARM_USB_PID_SETUP : Driver_USB.h
- ARM_USB_PID_SOF : Driver_USB.h
- ARM_USB_PID_SPLIT : Driver_USB.h
- ARM_USB_PID_STALL : Driver_USB.h
- ARM_USB_PIN_DM : Driver_USB.h
- ARM_USB_PIN_DP : Driver_USB.h
- ARM_USB_PIN_ID : Driver_USB.h
- ARM_USB_PIN_OC : Driver_USB.h
- ARM_USB_PIN_VBUS : Driver_USB.h
- ARM_USB_ROLE_DEVICE : Driver_USB.h
- ARM_USB_ROLE_HOST : Driver_USB.h
- ARM_USB_ROLE_NONE : Driver_USB.h
- ARM_USB_SPEED_FULL : Driver_USB.h
- ARM_USB_SPEED_HIGH : Driver_USB.h
- ARM_USB_SPEED_LOW : Driver_USB.h
- ARM_USBD_API_VERSION : Driver_USBD.h
- ARM_USBD_DeviceConnect() : Driver_USBD.c
- ARM_USBD_DeviceDisconnect() : Driver_USBD.c
- ARM_USBD_DeviceGetState() : Driver_USBD.c
- ARM_USBD_DeviceRemoteWakeup() : Driver_USBD.c
- ARM_USBD_DeviceSetAddress() : Driver_USBD.c
- ARM_USBD_EndpointConfigure() : Driver_USBD.c
- ARM_USBD_EndpointStall() : Driver_USBD.c
- ARM_USBD_EndpointTransfer() : Driver_USBD.c
- ARM_USBD_EndpointTransferAbort() : Driver_USBD.c
- ARM_USBD_EndpointTransferGetResult() : Driver_USBD.c
- ARM_USBD_EndpointUnconfigure() : Driver_USBD.c
- ARM_USBD_EVENT_HIGH_SPEED : Driver_USBD.h
- ARM_USBD_EVENT_IN : Driver_USBD.h
- ARM_USBD_EVENT_OUT : Driver_USBD.h
- ARM_USBD_EVENT_RESET : Driver_USBD.h
- ARM_USBD_EVENT_RESUME : Driver_USBD.h
- ARM_USBD_EVENT_SETUP : Driver_USBD.h
- ARM_USBD_EVENT_SUSPEND : Driver_USBD.h
- ARM_USBD_EVENT_VBUS_OFF : Driver_USBD.h
- ARM_USBD_EVENT_VBUS_ON : Driver_USBD.h
- ARM_USBD_GetCapabilities() : Driver_USBD.c
- ARM_USBD_GetFrameNumber() : Driver_USBD.c
- ARM_USBD_GetVersion() : Driver_USBD.c
- ARM_USBD_Initialize() : Driver_USBD.c
- ARM_USBD_PowerControl() : Driver_USBD.c
- ARM_USBD_ReadSetupPacket() : Driver_USBD.c
- ARM_USBD_SignalDeviceEvent() : Driver_USBD.c
- ARM_USBD_SignalDeviceEvent_t : Driver_USBD.h
- ARM_USBD_SignalEndpointEvent() : Driver_USBD.c
- ARM_USBD_SignalEndpointEvent_t : Driver_USBD.h
- ARM_USBD_Uninitialize() : Driver_USBD.c
- ARM_USBH_API_VERSION : Driver_USBH.h
- ARM_USBH_EP_HANDLE : Driver_USBH.h
- ARM_USBH_EVENT_BUS_ERROR : Driver_USBH.h
- ARM_USBH_EVENT_CONNECT : Driver_USBH.h
- ARM_USBH_EVENT_DISCONNECT : Driver_USBH.h
- ARM_USBH_EVENT_HANDSHAKE_ERR : Driver_USBH.h
- ARM_USBH_EVENT_HANDSHAKE_MDATA : Driver_USBH.h
- ARM_USBH_EVENT_HANDSHAKE_NAK : Driver_USBH.h
- ARM_USBH_EVENT_HANDSHAKE_NYET : Driver_USBH.h
- ARM_USBH_EVENT_HANDSHAKE_STALL : Driver_USBH.h
- ARM_USBH_EVENT_OVERCURRENT : Driver_USBH.h
- ARM_USBH_EVENT_REMOTE_WAKEUP : Driver_USBH.h
- ARM_USBH_EVENT_RESET : Driver_USBH.h
- ARM_USBH_EVENT_RESUME : Driver_USBH.h
- ARM_USBH_EVENT_SUSPEND : Driver_USBH.h
- ARM_USBH_EVENT_TRANSFER_COMPLETE : Driver_USBH.h
- ARM_USBH_GetCapabilities() : Driver_USBH.c
- ARM_USBH_GetFrameNumber() : Driver_USBH.c
- ARM_USBH_GetVersion() : Driver_USBH.c
- ARM_USBH_HCI_GetCapabilities() : Driver_USBH.c
- ARM_USBH_HCI_GetVersion() : Driver_USBH.c
- ARM_USBH_HCI_Initialize() : Driver_USBH.c
- ARM_USBH_HCI_Interrupt() : Driver_USBH.c
- ARM_USBH_HCI_Interrupt_t : Driver_USBH.h
- ARM_USBH_HCI_PortVbusOnOff() : Driver_USBH.c
- ARM_USBH_HCI_PowerControl() : Driver_USBH.c
- ARM_USBH_HCI_Uninitialize() : Driver_USBH.c
- ARM_USBH_Initialize() : Driver_USBH.c
- ARM_USBH_PACKET_CSPLIT : Driver_USBH.h
- ARM_USBH_PACKET_DATA0 : Driver_USBH.h
- ARM_USBH_PACKET_DATA1 : Driver_USBH.h
- ARM_USBH_PACKET_DATA_Msk : Driver_USBH.h
- ARM_USBH_PACKET_DATA_Pos : Driver_USBH.h
- ARM_USBH_PACKET_IN : Driver_USBH.h
- ARM_USBH_PACKET_OUT : Driver_USBH.h
- ARM_USBH_PACKET_PING : Driver_USBH.h
- ARM_USBH_PACKET_PRE : Driver_USBH.h
- ARM_USBH_PACKET_SETUP : Driver_USBH.h
- ARM_USBH_PACKET_SPLIT_Msk : Driver_USBH.h
- ARM_USBH_PACKET_SPLIT_Pos : Driver_USBH.h
- ARM_USBH_PACKET_SSPLIT : Driver_USBH.h
- ARM_USBH_PACKET_SSPLIT_E : Driver_USBH.h
- ARM_USBH_PACKET_SSPLIT_S : Driver_USBH.h
- ARM_USBH_PACKET_SSPLIT_S_E : Driver_USBH.h
- ARM_USBH_PACKET_TOKEN_Msk : Driver_USBH.h
- ARM_USBH_PACKET_TOKEN_Pos : Driver_USBH.h
- ARM_USBH_PIPE_HANDLE : Driver_USBH.h
- ARM_USBH_PipeCreate() : Driver_USBH.c
- ARM_USBH_PipeDelete() : Driver_USBH.c
- ARM_USBH_PipeModify() : Driver_USBH.c
- ARM_USBH_PipeReset() : Driver_USBH.c
- ARM_USBH_PipeTransfer() : Driver_USBH.c
- ARM_USBH_PipeTransferAbort() : Driver_USBH.c
- ARM_USBH_PipeTransferGetResult() : Driver_USBH.c
- ARM_USBH_PortGetState() : Driver_USBH.c
- ARM_USBH_PortReset() : Driver_USBH.c
- ARM_USBH_PortResume() : Driver_USBH.c
- ARM_USBH_PortSuspend() : Driver_USBH.c
- ARM_USBH_PortVbusOnOff() : Driver_USBH.c
- ARM_USBH_PowerControl() : Driver_USBH.c
- ARM_USBH_SignalEndpointEvent_t : Driver_USBH.h
- ARM_USBH_SignalPipeEvent() : Driver_USBH.c
- ARM_USBH_SignalPipeEvent_t : Driver_USBH.h
- ARM_USBH_SignalPortEvent() : Driver_USBH.c
- ARM_USBH_SignalPortEvent_t : Driver_USBH.h
- ARM_USBH_Uninitialize() : Driver_USBH.c