CMSIS-Driver: Status Error Codes

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
Status Error Codes
SAI Interface

Negative values indicate errors (SAI has specific codes in addition to common Status Error Codes). More...

## Macros
#define | ARM_SAI_ERROR_SYNCHRONIZATION (ARM_DRIVER_ERROR_SPECIFIC - 1)
| Specified Synchronization not supported. More...
#define | ARM_SAI_ERROR_PROTOCOL (ARM_DRIVER_ERROR_SPECIFIC - 2)
| Specified Protocol not supported. More...
#define | ARM_SAI_ERROR_DATA_SIZE (ARM_DRIVER_ERROR_SPECIFIC - 3)
| Specified Data size not supported. More...
#define | ARM_SAI_ERROR_BIT_ORDER (ARM_DRIVER_ERROR_SPECIFIC - 4)
| Specified Bit order not supported. More...
#define | ARM_SAI_ERROR_MONO_MODE (ARM_DRIVER_ERROR_SPECIFIC - 5)
| Specified Mono mode not supported. More...
#define | ARM_SAI_ERROR_COMPANDING (ARM_DRIVER_ERROR_SPECIFIC - 6)
| Specified Companding not supported. More...
#define | ARM_SAI_ERROR_CLOCK_POLARITY (ARM_DRIVER_ERROR_SPECIFIC - 7)
| Specified Clock polarity not supported. More...
#define | ARM_SAI_ERROR_AUDIO_FREQ (ARM_DRIVER_ERROR_SPECIFIC - 8)
| Specified Audio frequency not supported. More...
#define | ARM_SAI_ERROR_MCLK_PIN (ARM_DRIVER_ERROR_SPECIFIC - 9)
| Specified MCLK Pin setting not supported. More...
#define | ARM_SAI_ERROR_MCLK_PRESCALER (ARM_DRIVER_ERROR_SPECIFIC - 10)
| Specified MCLK Prescaler not supported. More...
#define | ARM_SAI_ERROR_FRAME_LENGHT (ARM_DRIVER_ERROR_SPECIFIC - 11)
| Specified Frame length not supported. More...
#define | ARM_SAI_ERROR_FRAME_SYNC_WIDTH (ARM_DRIVER_ERROR_SPECIFIC - 12)
| Specified Frame Sync width not supported. More...
#define | ARM_SAI_ERROR_FRAME_SYNC_POLARITY (ARM_DRIVER_ERROR_SPECIFIC - 13)
| Specified Frame Sync polarity not supported. More...
#define | ARM_SAI_ERROR_FRAME_SYNC_EARLY (ARM_DRIVER_ERROR_SPECIFIC - 14)
| Specified Frame Sync early not supported. More...
#define | ARM_SAI_ERROR_SLOT_COUNT (ARM_DRIVER_ERROR_SPECIFIC - 15)
| Specified Slot count not supported. More...
#define | ARM_SAI_ERROR_SLOT_SIZE (ARM_DRIVER_ERROR_SPECIFIC - 16)
| Specified Slot size not supported. More...
#define | ARM_SAI_ERROR_SLOT_OFFESET (ARM_DRIVER_ERROR_SPECIFIC - 17)
| Specified Slot offset not supported. More...

## Description

Negative values indicate errors (SAI has specific codes in addition to common Status Error Codes).

The SAI driver has additional status error codes that are listed below.

Note
  - In case multiple errors exist, only the first encountered error will be reported.
  - errors ARM_SAI_ERROR_BIT_ORDER, ARM_SAI_ERROR_FRAME_SYNC_xxx, ARM_SAI_ERROR_SLOT_xxx will only be reported in User Defined Protocol mode.
  - The SAI driver also returns the common Status Error Codes.

## Macro Definition Documentation

#define ARM_SAI_ERROR_SYNCHRONIZATION (ARM_DRIVER_ERROR_SPECIFIC - 1)

Specified Synchronization not supported.

The synchronization requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_PROTOCOL (ARM_DRIVER_ERROR_SPECIFIC - 2)

Specified Protocol not supported.

The protocol requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_DATA_SIZE (ARM_DRIVER_ERROR_SPECIFIC - 3)

Specified Data size not supported.

The data size requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_BIT_ORDER (ARM_DRIVER_ERROR_SPECIFIC - 4)

Specified Bit order not supported.

The bit order requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_MONO_MODE (ARM_DRIVER_ERROR_SPECIFIC - 5)

Specified Mono mode not supported.

The mono mode requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_COMPANDING (ARM_DRIVER_ERROR_SPECIFIC - 6)

Specified Companding not supported.

The companding requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_CLOCK_POLARITY (ARM_DRIVER_ERROR_SPECIFIC - 7)

Specified Clock polarity not supported.

The clock polarity requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_AUDIO_FREQ (ARM_DRIVER_ERROR_SPECIFIC - 8)

Specified Audio frequency not supported.

The audio frequency requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_MCLK_PIN (ARM_DRIVER_ERROR_SPECIFIC - 9)

Specified MCLK Pin setting not supported.

The MCLK pin setting requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_MCLK_PRESCALER (ARM_DRIVER_ERROR_SPECIFIC - 10)

Specified MCLK Prescaler not supported.

The MCLK prescaler requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_FRAME_LENGHT (ARM_DRIVER_ERROR_SPECIFIC - 11)

Specified Frame length not supported.

The frame length requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_FRAME_SYNC_WIDTH (ARM_DRIVER_ERROR_SPECIFIC - 12)

Specified Frame Sync width not supported.

The frame sync width requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_FRAME_SYNC_POLARITY (ARM_DRIVER_ERROR_SPECIFIC - 13)

Specified Frame Sync polarity not supported.

The frame sync polarity requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_FRAME_SYNC_EARLY (ARM_DRIVER_ERROR_SPECIFIC - 14)

Specified Frame Sync early not supported.

The frame sync early requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_SLOT_COUNT (ARM_DRIVER_ERROR_SPECIFIC - 15)

Specified Slot count not supported.

The slot count requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_SLOT_SIZE (ARM_DRIVER_ERROR_SPECIFIC - 16)

Specified Slot size not supported.

The slot size requested with the function ARM_SAI_Control is not supported.

#define ARM_SAI_ERROR_SLOT_OFFESET (ARM_DRIVER_ERROR_SPECIFIC - 17)

Specified Slot offset not supported.

The slot offset requested with the function ARM_SAI_Control is not supported.