/**
  @page WWDG_RefreshUntilUserEvent WWDG example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    Examples_LL/WWDG/WWDG_RefreshUntilUserEvent/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the WWDG_RefreshUntilUserEvent example.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright (c) 2016 STMicroelectronics.
  * All rights reserved.</center></h2>
  *
  * This software component is licensed by ST under BSD 3-Clause license,
  * the "License"; You may not use this file except in compliance with the
  * License. You may obtain a copy of the License at:
  *                        opensource.org/licenses/BSD-3-Clause
  *
  ******************************************************************************
  @endverbatim

@par Example Description

Configuration of the WWDG to periodically update the counter and 
generate an MCU WWDG reset when a user button is pressed. The peripheral initialization 
uses the LL unitary service functions for optimization purposes (performance and size).

Example Configuration:
Configure the WWDG (Window, Prescaler & Counter) and enable it.
Refresh the WWDG downcounter in the main loop - Led is blinking fastly & continuously

Example Execution:
When User Button is pressed, the Downcounter automatic refresh mechanism is disable and thus, reset will occur.
After a reset when re-entering in the main, RCC WWDG Reset Flag will be checked and if we are back from a WWDG reset the led will be switch ON.

Waiting a new user button pressed to re-activate the WWDG

@par Directory contents 

  - WWDG/WWDG_RefreshUntilUserEvent/Inc/stm32f0xx_it.h          Interrupt handlers header file
  - WWDG/WWDG_RefreshUntilUserEvent/Inc/main.h                  Header for main.c module
  - WWDG/WWDG_RefreshUntilUserEvent/Inc/stm32_assert.h          Template file to include assert_failed function
  - WWDG/WWDG_RefreshUntilUserEvent/Src/stm32f0xx_it.c          Interrupt handlers
  - WWDG/WWDG_RefreshUntilUserEvent/Src/main.c                  Main program
  - WWDG/WWDG_RefreshUntilUserEvent/Src/system_stm32f0xx.c      STM32F0xx system source file


@par Hardware and Software environment

  - This example runs on STM32F072xB devices.
    
  - This example has been tested with STM32F072RB-Nucleo RevC board and can be
    easily tailored to any other supported device and development board.


@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
