/**
  @page DMA_CopyFromFlashToMemory DMA example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    Examples_LL/DMA/DMA_CopyFromFlashToMemory/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the DMA example.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright (c) 2016 STMicroelectronics.
  * All rights reserved.</center></h2>
  *
  * This software component is licensed by ST under BSD 3-Clause license,
  * the "License"; You may not use this file except in compliance with the
  * License. You may obtain a copy of the License at:
  *                        opensource.org/licenses/BSD-3-Clause
  *
  ******************************************************************************
  @endverbatim

@par Example Description

How to use a DMA channel to transfer a word data buffer
from Flash memory to embedded SRAM. The peripheral initialization uses 
LL unitary service functions for optimization purposes (performance and size).

At the beginning of the main program the SystemClock_Config() function is used to configure the system
clock (SYSCLK) to run at 48 MHz.

Then the LED_Init() function is used to initialize the LED2.

Then the Configure_DMA() function is used to configure the DMA1_Channel1 to transfer the contents of a 32-word data 
buffer stored in Flash memory to the reception buffer declared in RAM.

The start of transfer is triggered by software(LL_DMA_EnableChannel()). DMA1_Channel1 memory-to-memory
transfer is enabled. Source and destination addresses incrementing is also enabled.
The transfer is started by setting the channel enable bit for DMA1_Channel1.
At the end of the transfer a Transfer Complete interrupt is generated since it
is enabled and the callback function (customized by user) is called.

Finally, aSRC_Const_Buffer and aDST_Buffer are compared through Buffercmp() in order to 
check buffers correctness.  

STM32F072RB-Nucleo RevC's LED can be used to monitor the transfer status:
- LED2 is turn on if DMA data transferred consistency.
- LED2 is blinking every 1 sec in case of error.

@par Directory contents 

  - DMA/DMA_CopyFromFlashToMemory/Inc/stm32f0xx_it.h          Interrupt handlers header file
  - DMA/DMA_CopyFromFlashToMemory/Inc/main.h                  Header for main.c module  
  - DMA/DMA_CopyFromFlashToMemory/Inc/stm32_assert.h          Template file to include assert_failed function
  - DMA/DMA_CopyFromFlashToMemory/Src/stm32f0xx_it.c          Interrupt handlers
  - DMA/DMA_CopyFromFlashToMemory/Src/main.c                  Main program
  - DMA/DMA_CopyFromFlashToMemory/Src/system_stm32f0xx.c      STM32F0xx system source file

@par Hardware and Software environment

  - This example runs on STM32F072xB devices.
    
  - This example has been tested with STM32F072RB-Nucleo RevC board and can be
    easily tailored to any other supported device and development board.


@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
