CMSIS-Core (Cortex-M): Register Mapping

| CMSIS-Core (Cortex-M) Version 5.1.2 CMSIS-Core support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Register Mapping

The table below associates some common register names used in CMSIS to the register names used in Technical Reference Manuals.

CMSIS Register Name | Cortex-M3, Cortex-M4, and Cortex-M7 | Cortex-M0 and Cortex-M0+ | Register Name
--- | --- | --- | ---
Nested Vectored Interrupt Controller (NVIC) Register Access
NVIC->ISER[] | NVIC_ISER0..7 | ISER | Interrupt Set-Enable Registers
NVIC->ICER[] | NVIC_ICER0..7 | ICER | Interrupt Clear-Enable Registers
NVIC->ISPR[] | NVIC_ISPR0..7 | ISPR | Interrupt Set-Pending Registers
NVIC->ICPR[] | NVIC_ICPR0..7 | ICPR | Interrupt Clear-Pending Registers
NVIC->IABR[] | NVIC_IABR0..7 | - | Interrupt Active Bit Register
NVIC->IP[] | NVIC_IPR0..59 | IPR0..7 | Interrupt Priority Register
NVIC->STIR | STIR | - | Software Triggered Interrupt Register
System Control Block (SCB) Register Access
SCB->CPUID | CPUID | CPUID | CPUID Base Register
SCB->ICSR | ICSR | ICSR | Interrupt Control and State Register
SCB->VTOR | VTOR | - | Vector Table Offset Register
SCB->AIRCR | AIRCR | AIRCR | Application Interrupt and Reset Control Register
SCB->SCR | SCR | SCR | System Control Register
SCB->CCR | CCR | CCR | Configuration and Control Register
SCB->SHP[] | SHPR1..3 | SHPR2..3 | System Handler Priority Registers
SCB->SHCSR | SHCSR | SHCSR | System Handler Control and State Register
SCB->CFSR | CFSR | - | Configurable Fault Status Registers
SCB->HFSR | HFSR | - | HardFault Status Register
SCB->DFSR | DFSR | - | Debug Fault Status Register
SCB->MMFAR | MMFAR | - | MemManage Fault Address Register
SCB->BFAR | BFAR | - | BusFault Address Register
SCB->AFSR | AFSR | - | Auxiliary Fault Status Register
SCB->PFR[] | ID_PFR0..1 | - | Processor Feature Registers
SCB->DFR | ID_DFR0 | - | Debug Feature Register
SCB->ADR | ID_AFR0 | - | Auxiliary Feature Register
SCB->MMFR[] | ID_MMFR0..3 | - | Memory Model Feature Registers
SCB->ISAR[] | ID_ISAR0..4 | - | Instruction Set Attributes Registers
SCB->CPACR | CPACR | - | Coprocessor Access Control Register
System Control and ID Registers not in the SCB (SCnSCB) Register Access
SCnSCB->ICTR | ICTR | - | Interrupt Controller Type Register
SCnSCB->ACTLR | ACTLR | - | Auxiliary Control Register
System Timer (SysTick) Control and Status Register Access
SysTick->CTRL | STCSR | SYST_CSR | SysTick Control and Status Register
SysTick->LOAD | STRVR | SYST_RVR | SysTick Reload Value Register
SysTick->VAL | STCVR | SYST_CVR | SysTick Current Value Register
SysTick->CALIB | STCR | SYST_CALIB | SysTick Calibaration Value Register
Data Watchpoint and Trace (DWT) Register Access
DWT->CTRL | DWT_CTRL | - | Control Register
DWT->CYCCNT | DWT_CYCCNT | - | Cycle Count Register
DWT->CPICNT | DWT_CPICNT | - | CPI Count Register
DWT->EXCCNT | DWT_EXCCNT | - | Exception Overhead Count Register
DWT->SLEEPCNT | DWT_SLEEPCNT | - | Sleep Count Register
DWT->LSUCNT | DWT_LSUCNT | - | LSU Count Register
DWT->FOLDCNT | DWT_FOLDCNT | - | Folded-instruction Count Register
DWT->PCSR | DWT_PCSR | - | Program Counter Sample Register
DWT->COMP0..3 | DWT_COMP0..3 | - | Comparator Register 0..3
DWT->MASK0..3 | DWT_MASK0..3 | - | Mask Register 0..3
DWT->FUNCTION0..3 | DWT_FUNCTION0..3 | - | Function Register 0..3
Instrumentation Trace Macrocell (ITM) Register Access
ITM->PORT[] | ITM_STIM0..31 | - | Stimulus Port Registers
ITM->TER | ITM_TER | - | Trace Enable Register
ITM->TPR | ITM_TPR | - | ITM Trace Privilege Register
ITM->TCR | ITM_TCR | - | Trace Control Register
Trace Port Interface (TPIU) Register Access
TPI->SSPSR | TPIU_SSPR | - | Supported Parallel Port Size Register
TPI->CSPSR | TPIU_CSPSR | - | Current Parallel Port Size Register
TPI->ACPR | TPIU_ACPR | - | Asynchronous Clock Prescaler Register
TPI->SPPR | TPIU_SPPR | - | Selected Pin Protocol Register
TPI->FFSR | TPIU_FFSR | - | Formatter and Flush Status Register
TPI->FFCR | TPIU_FFCR | - | Formatter and Flush Control Register
TPI->FSCR | TPIU_FSCR | - | Formatter Synchronization Counter Register
TPI->TRIGGER | TRIGGER | - | TRIGGER
TPI->FIFO0 | FIFO data 0 | - | Integration ETM Data
TPI->ITATBCTR2 | ITATBCTR2 | - | ITATBCTR2
TPI->ITATBCTR0 | ITATBCTR0 | - | ITATBCTR0
TPI->FIFO1 | FIFO data 1 | - | Integration ITM Data
TPI->ITCTRL | TPIU_ITCTRL | - | Integration Mode Control
TPI->CLAIMSET | CLAIMSET | - | Claim tag set
TPI->CLAIMCLR | CLAIMCLR | - | Claim tag clear
TPI->DEVID | TPIU_DEVID | - | TPIU_DEVID
TPI->DEVTYPE | TPIU_DEVTYPE | - | TPIU_DEVTYPE
Memory Protection Unit (MPU) Register Access
MPU->TYPE | MPU_TYPE | - | MPU Type Register
MPU->CTRL | MPU_CTRL | - | MPU Control Register
MPU->RNR | MPU_RNR | - | MPU Region Number Register
MPU->RBAR | MPU_RBAR | - | MPU Region Base Address Register
MPU->RASR | MPU_RASR | - | MPU Region Attribute and Size Register
MPU->RBAR_A1..3 | MPU_RBAR_A1..3 | - | MPU alias Register
MPU->RSAR_A1..3 | MPU_RSAR_A1..3 | - | MPU alias Register
Floating Point Unit (FPU) Register Access [only Cortex-M4 and Cortex-M7 both with FPU]
FPU->FPCCR | FPCCR | - | FP Context Control Register
FPU->FPCAR | FPCAR | - | FP Context Address Register
FPU->FPDSCR | FPDSCR | - | FP Default Status Control Register
FPU->MVFR0..1 | MVFR0..1 | - | Media and VFP Feature Registers