CMSIS-Driver: I2C Address Flags

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
I2C Address Flags
I2C Interface

Specify address flags. More...

## Macros
#define | ARM_I2C_ADDRESS_10BIT (0x0400)
| 10-bit address flag More...
#define | ARM_I2C_ADDRESS_GC (0x8000)
| General Call flag. More...

## Description

Specify address flags.

Specifies the address type for the functions ARM_I2C_MasterReceive, ARM_I2C_MasterTransmit and ARM_I2C_OWN_ADDRESS.

## Macro Definition Documentation

#define ARM_I2C_ADDRESS_10BIT (0x0400)

10-bit address flag

See Also
  ARM_I2C_OWN_ADDRESS
  ARM_I2C_MasterTransmit
  ARM_I2C_MasterReceive

#define ARM_I2C_ADDRESS_GC (0x8000)

General Call flag.

See Also
  ARM_I2C_OWN_ADDRESS