Back to Release page
# Release Notes for STM32072B_EVAL Applications Copyright 2016 STMicroelectronics
## Update History ### V1.11.0 / 12-September-2019 Main Changes Update for compatibility with FreeRTOS v10.0.1_20190329 Update for compatibility with TouchSensing v2.2.4 Update for compatibility with USB Device v2.5.3 Update stm32f0xx_hal_conf.h files : Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Add reference to HAL EXTI driver Add registers callbacks defines ### V1.9.0 / 25-August-2017 Main Changes Maintenance release. Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Add a note in DFU example readme : "How to instal Dfuse demo under Window 8.1". Align stm32f0xx_hal_conf.h with latest template defined in HAL. Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Remove Cortex-M3/M4 specific defines and macros in FreeRTOSConfig.h from all FreeRTOS based applications. ### V1.8.0 / 07-April-2017 Main Changes Maintenance release Update stm32f0xx_hal_conf.h files : Compliancy with MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). Add definition of USE_SPI_CRC Update FreeRTOS_Semaphore and FreeRTOS_ThreadCreation examples to be aligned with latest reference code. ### V1.7.0 / 04-November-2016 Main Changes Maintenance release USB : Added suffix "U" to FLASH_PAGE_SIZE in usbd_conf.h Change in HAL API for TIM : add AutoReloadPreload capability in TIM handler. Impacts in USB Device example and in all FreeRTOS examples Updated FreeRTOS examples to call TIM HW function as time base source instead of Systick ; changes in following examples : FreeRTOS Low Power FreeRTOS Mutexes FreeRTOS_Queues FreeRTOS Semaphore FreeRTOS Thread Creation FreeRTOS Timers ### V1.6.0 / 27-May-2016 Main Changes Maintenance release. Updated system_stm32f0xx.c files: Added APBPrescTable definition. Updated HEAP size for FreeRTOS applications (updates in FreeRTOSConfig.h). Updated HEAP size for USB_Device/MSC_Standalone application. ### V1.5.0 / 29-January-2016 Main Changes Maintenance release. Add support of System Workbench for STM32 (SW4STM32) toolchain. Updated GPIO Output Speed literals naming to ensure HAL full compatibility. Updated system_stm32f0xx.c files: Removed __IO or __I on constant table declaration. Added HSI48_VALUE definition. Updated stm32f0xx_hal_conf.h files: Set HSE_STARTUP_TIMEOUT value to 100ms instead of 5000ms Updated “Liberty” License with the new license “Ultimate Liberty”. ### V1.3.0 / 26-June-2015 Main Changes Adapt existing projects to use FreeRTOS V8.2.1. Upgrade to use FatFs R0.11. Update USB application projects. Fix known defects and several enhancements implementation. Complete HAL API alignment (renaming). ### V1.2.0 / 05-Dec-2014 Main Changes Update for compatibility with: FatFS R0.10b_STM32Cube_20141120 USB_device V2.3.0 FreeRTOS V8.1.2_20141204 ### V1.0.0 / 18-Juin-2014 Main Changes First official release. ## License This software component is licensed by ST under Ultimate Liberty license SLA0044, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/SLA0044 For complete documentation on STM32 Microcontrollers visit www.st.com/STM32