CMSIS-Core (Cortex-M): Intrinsic Functions for CPU Instructions

| CMSIS-Core (Cortex-M) Version 5.1.2 CMSIS-Core support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Functions
Intrinsic Functions for CPU Instructions

Functions that generate specific Cortex-M CPU Instructions. More...

## Functions
void | __NOP (void)
| No Operation. More...
void | __WFI (void)
| Wait For Interrupt. More...
void | __WFE (void)
| Wait For Event. More...
void | __SEV (void)
| Send Event. More...
void | __BKPT (uint8_t value)
| Set Breakpoint. More...
void | __ISB (void)
| Instruction Synchronization Barrier. More...
void | __DSB (void)
| Data Synchronization Barrier. More...
void | __DMB (void)
| Data Memory Barrier. More...
uint32_t | __REV (uint32_t value)
| Reverse byte order (32 bit) More...
uint32_t | __REV16 (uint32_t value)
| Reverse byte order (16 bit) More...
int32_t | __REVSH (int32_t value)
| Reverse byte order (16 bit) More...
uint32_t | __RBIT (uint32_t value)
| Reverse bit order of value. More...
uint32_t | __ROR (uint32_t value, uint32_t shift)
| Rotate a value right by a number of bits. More...
uint8_t | __LDREXB (volatile uint8_t *addr)
| LDR Exclusive (8 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint16_t | __LDREXH (volatile uint16_t *addr)
| LDR Exclusive (16 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint32_t | __LDREXW (volatile uint32_t *addr)
| LDR Exclusive (32 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint32_t | __STREXB (uint8_t value, volatile uint8_t *addr)
| STR Exclusive (8 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint32_t | __STREXH (uint16_t value, volatile uint16_t *addr)
| STR Exclusive (16 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint32_t | __STREXW (uint32_t value, volatile uint32_t *addr)
| STR Exclusive (32 bit) [not for Cortex-M0, Cortex-M0+, or SC000]. More...
void | __CLREX (void)
| Remove the exclusive lock [not for Cortex-M0, Cortex-M0+, or SC000]. More...
int32_t | __SSAT (int32_t value, uint32_t sat)
| Signed Saturate [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint32_t | __USAT (uint32_t value, uint32_t sat)
| Unsigned Saturate [not for Cortex-M0, Cortex-M0+, or SC000]. More...
uint8_t | __CLZ (uint32_t value)
| Count leading zeros. More...
uint32_t | __RRX (uint32_t value)
| Rotate Right with Extend (32 bit) More...
uint8_t | __LDRBT (uint8_t ptr)
| LDRT Unprivileged (8 bit) More...
uint16_t | __LDRHT (uint16_t ptr)
| LDRT Unprivileged (16 bit) More...
uint32_t | __LDRT (uint32_t ptr)
| LDRT Unprivileged (32 bit) More...
void | __STRBT (uint8_t value, uint8_t ptr)
| STRT Unprivileged (8 bit) More...
void | __STRHT (uint16_t value, uint16_t ptr)
| STRT Unprivileged (16 bit) More...
void | __STRT (uint32_t value, uint32_t ptr)
| STRT Unprivileged (32 bit) More...
uint8_t | __LDAB (volatile uint8_t *ptr)
| Load-Acquire (8 bit) More...
uint16_t | __LDAH (volatile uint16_t *ptr)
| Load-Acquire (16 bit) More...
uint32_t | __LDA (volatile uint32_t *ptr)
| Load-Acquire (32 bit) More...
void | __STLB (uint8_t value, volatile uint8_t *ptr)
| Store-Release (8 bit) More...
void | __STLH (uint16_t value, volatile uint16_t *ptr)
| Store-Release (16 bit) More...
void | __STL (uint32_t value, volatile uint32_t *ptr)
| Store-Release (32 bit) More...
uint8_t | __LDAEXB (volatile uint32_t *ptr)
| Load-Acquire Exclusive (8 bit) More...
uint16_t | __LDAEXH (volatile uint32_t *ptr)
| Load-Acquire Exclusive (16 bit) More...
uint32_t | __LDAEX (volatile uint32_t *ptr)
| Load-Acquire Exclusive (32 bit) More...
uint32_t | __STLEXB (uint8_t value, volatile uint8_t *ptr)
| Store-Release Exclusive (8 bit) More...
uint32_t | __STLEXH (uint16_t value, volatile uint16_t *ptr)
| Store-Release Exclusive (16 bit) More...
uint32_t | __STLEX (uint32_t value, volatile uint32_t *ptr)
| Store-Release Exclusive (32 bit) More...

## Description

The following functions generate specific Cortex-M instructions that cannot be directly accessed by the C/C++ Compiler. Refer to the Cortex-M Reference Manuals for detailed information about these Cortex-M instructions.

Note
  When using the Arm Compiler Version 5 Toolchain the following Intrinsic Functions for CPU Instructions are implemented using the Embedded Assembler. As the Embedded Assembler may cause side effects (Refer to Arm Compiler v5.xx User Guide - Using the Inline and Embedded Assemblers of the Arm Compiler for more information) it is possible to disable the following intrinsic functions and therefore the usage of the Embedded Assembler with the define __NO_EMBEDDED_ASM:
  - __REV16
  - __REVSH
  - __RRX

## Function Documentation

void __BKPT | ( | uint8_t | value | ) |

This function causes the processor to enter Debug state. Debug tools can use this to investigate system state when the instruction at a particular address is reached.

Parameters

  [in] | value | is ignored by the processor. If required, a debugger can use it to obtain additional information about the breakpoint.

void __CLREX | ( | void |  | ) |

This function removes the exclusive lock which is created by LDREX [not for Cortex-M0, Cortex-M0+, or SC000].

uint8_t __CLZ | ( | uint32_t | value | ) |

This function counts the number of leading zeros of a data value.

On Armv6-M (Cortex-M0, Cortex-M0+, and SC000) this function is not available as a core instruction instruction and thus __CLZ is implemented in software.

Parameters

  [in] | value | Value to count the leading zeros

Returns
  number of leading zeros in value

void __DMB | ( | void |  | ) |

This function ensures the apparent order of the explicit memory operations before and after the instruction, without ensuring their completion.

void __DSB | ( | void |  | ) |

This function acts as a special kind of Data Memory Barrier. It completes when all explicit memory accesses before this instruction complete.

void __ISB | ( | void |  | ) |

Instruction Synchronization Barrier flushes the pipeline in the processor, so that all instructions following the ISB are fetched from cache or memory, after the instruction has been completed.

uint32_t __LDA | ( | volatile uint32_t * | ptr | ) |

Executes a LDA instruction for 32 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint32_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint8_t __LDAB | ( | volatile uint8_t * | ptr | ) |

Executes a LDAB instruction for 8 bit value.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint8_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint32_t __LDAEX | ( | volatile uint32_t * | ptr | ) |

Executes a LDA exclusive instruction for 32 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint32_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint8_t __LDAEXB | ( | volatile uint32_t * | ptr | ) |

Executes a LDAB exclusive instruction for 8 bit value.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint8_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint16_t __LDAEXH | ( | volatile uint32_t * | ptr | ) |

Executes a LDAH exclusive instruction for 16 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint16_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint16_t __LDAH | ( | volatile uint16_t * | ptr | ) |

Executes a LDAH instruction for 16 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint16_t at (*ptr)

Note
  Only availabe for Armv8-M Architecture.

uint8_t __LDRBT | ( | uint8_t | ptr | ) |

This function executed an Unprivileged LDRT command for 8 bit value.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint8_t at (*ptr)

uint8_t __LDREXB | ( | volatile uint8_t * | addr | ) |

This function executed an exclusive LDR command for 8 bit value [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | *addr | Pointer to data

Returns
  value of type uint8_t at (*addr)

uint16_t __LDREXH | ( | volatile uint16_t * | addr | ) |

This function executed an exclusive LDR command for 16 bit values [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | *addr | Pointer to data

Returns
  value of type uint16_t at (*addr)

uint32_t __LDREXW | ( | volatile uint32_t * | addr | ) |

This function executed an exclusive LDR command for 32 bit values [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | *addr | Pointer to data

Returns
  value of type uint32_t at (*addr)

uint16_t __LDRHT | ( | uint16_t | ptr | ) |

This function executed an Unprivileged LDRT command for 16 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint16_t at (*ptr)

uint32_t __LDRT | ( | uint32_t | ptr | ) |

This function executed an Unprivileged LDRT command for 32 bit values.

Parameters

  [in] | ptr | Pointer to data

Returns
  value of type uint32_t at (*ptr)

void __NOP | ( | void |  | ) |

This function does nothing. This instruction can be used for code alignment purposes.

uint32_t __RBIT | ( | uint32_t | value | ) |

Parameters

  [in] | value | Value to reverse

Returns
  Reversed value

uint32_t __REV | ( | uint32_t | value | ) |

Reverses the byte order in unsigned integer value. For example, 0x12345678 becomes 0x78563412.

Parameters

  [in] | value | Value to reverse

Returns
  Reversed value

uint32_t __REV16 | ( | uint32_t | value | ) |

Reverses the byte order within each halfword of a word. For example, 0x12345678 becomes 0x34127856.

Parameters

  [in] | value | Value to reverse

Returns
  Reversed value

int32_t __REVSH | ( | int32_t | value | ) |

Reverses the byte order in a 16-bit value and returns the signed 16-bit result. For example, 0x0080 becomes 0x8000.

Parameters

  [in] | value | Value to reverse

Returns
  Reversed value

uint32_t __ROR | ( | uint32_t | value,
|  | uint32_t | shift
| ) |  |

This function rotates a value right by a specified number of bits.

Parameters

  [in] | value | Value to be shifted right
  [in] | shift | Number of bits in the range [1..31]

Returns
  Rotated value

uint32_t __RRX | ( | uint32_t | value | ) |

This function moves each bit of a bitstring right by one bit. The carry input is shifted in at the left end of the bitstring.

Parameters

  [in] | value | Value to rotate

Returns
  Rotated value

void __SEV | ( | void |  | ) |

Send Event is a hint instruction. It causes an event to be signaled to the CPU.

int32_t __SSAT | ( | int32_t | value,
|  | uint32_t | sat
| ) |  |

This function saturates a signed value [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | value | Value to be saturated
  [in] | sat | Bit position to saturate to [1..32]

Returns
  Saturated value

void __STL | ( | uint32_t | value,
|  | volatile uint32_t * | ptr
| ) |  |

Executes a STL instruction for 32 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Note
  Only availabe for Armv8-M Architecture.

void __STLB | ( | uint8_t | value,
|  | volatile uint8_t * | ptr
| ) |  |

Executes a STLB instruction for 8 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Note
  Only availabe for Armv8-M Architecture.

uint32_t __STLEX | ( | uint32_t | value,
|  | volatile uint32_t * | ptr
| ) |  |

Executes a STL exclusive instruction for 32 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

Note
  Only availabe for Armv8-M Architecture.

uint32_t __STLEXB | ( | uint8_t | value,
|  | volatile uint8_t * | ptr
| ) |  |

Executes a STLB exclusive instruction for 8 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

Note
  Only availabe for Armv8-M Architecture.

uint32_t __STLEXH | ( | uint16_t | value,
|  | volatile uint16_t * | ptr
| ) |  |

Executes a STLH exclusive instruction for 16 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

Note
  Only availabe for Armv8-M Architecture.

void __STLH | ( | uint16_t | value,
|  | volatile uint16_t * | ptr
| ) |  |

Executes a STLH instruction for 16 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

Note
  Only availabe for Armv8-M Architecture.

void __STRBT | ( | uint8_t | value,
|  | uint8_t | ptr
| ) |  |

This function executed an Unprivileged STRT command for 8 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

uint32_t __STREXB | ( | uint8_t | value,
|  | volatile uint8_t * | addr
| ) |  |

This function executed an exclusive STR command for 8 bit values [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | value | Value to store
  [in] | *addr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

uint32_t __STREXH | ( | uint16_t | value,
|  | volatile uint16_t * | addr
| ) |  |

This function executed an exclusive STR command for 16 bit values [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | value | Value to store
  [in] | *addr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

uint32_t __STREXW | ( | uint32_t | value,
|  | volatile uint32_t * | addr
| ) |  |

This function executed an exclusive STR command for 32 bit values [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | value | Value to store
  [in] | *addr | Pointer to location

Returns
  0 Function succeeded
  1 Function failed

void __STRHT | ( | uint16_t | value,
|  | uint16_t | ptr
| ) |  |

This function executed an Unprivileged STRT command for 16 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

void __STRT | ( | uint32_t | value,
|  | uint32_t | ptr
| ) |  |

This function executed an Unprivileged STRT command for 32 bit values.

Parameters

  [in] | value | Value to store
  [in] | ptr | Pointer to location

uint32_t __USAT | ( | uint32_t | value,
|  | uint32_t | sat
| ) |  |

This function saturates an unsigned value [not for Cortex-M0, Cortex-M0+, or SC000].

Parameters

  [in] | value | Value to be saturated
  [in] | sat | Bit position to saturate to [0..31]

Returns
  Saturated value

void __WFE | ( | void |  | ) |

Wait For Event is a hint instruction that permits the processor to enter a low-power state until an events occurs:

- If the event register is 0, then WFE suspends execution until one of the following events occurs:
  - An exception, unless masked by the exception mask registers or the current priority level.
  - An exception enters the Pending state, if SEVONPEND in the System Control Register is set.
  - A Debug Entry request, if Debug is enabled.
  - An event signaled by a peripheral or another processor in a multiprocessor system using the SEV instruction.

- If the event register is 1, then WFE clears it to 0 and returns immediately.

void __WFI | ( | void |  | ) |

WFI is a hint instruction that suspends execution until one of the following events occurs:

- A non-masked interrupt occurs and is taken.
- An interrupt masked by PRIMASK becomes pending.
- A Debug Entry request.