CMSIS-Core (Cortex-A): Memory Management Unit Files mmu_<device>.c

| CMSIS-Core (Cortex-A) Version 1.1.2 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Memory Management Unit Files mmu_<device>.c

    /**************************************************************************//**
     * @file     system_Device.c
     * @brief    MMU Configuration
     *           Device <DeviceAbbreviation>
     * @version  V1.00
     * @date     10. January 2018
     ******************************************************************************/
    /*
     * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
     *
     * SPDX-License-Identifier: Apache-2.0
     *
     * Licensed under the Apache License, Version 2.0 (the License); you may
     * not use this file except in compliance with the License.
     * You may obtain a copy of the License at
     *
     * www.apache.org/licenses/LICENSE-2.0
     *
     * Unless required by applicable law or agreed to in writing, software
     * distributed under the License is distributed on an AS IS BASIS, WITHOUT
     * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
     * See the License for the specific language governing permissions and
     * limitations under the License.
     */

    /* Memory map description

       ToDo: add in this file your device memory map description
             following is an example of a Cortex-A9 Arm FVP device

                                                         Memory Type
    0xFFFFFFFF |--------------------------|             ------------
               |       FLAG SYNC          |             Device Memory
    0xFFFFF000 |--------------------------|             ------------
               |         Fault            |                Fault
    0xFFF00000 |--------------------------|             ------------
               |                          |                Normal
               |                          |
               |      Daughterboard       |
               |         memory           |
               |                          |
    0x80505000 |--------------------------|             ------------
               |TTB (L2 Sync Flags   ) 4k |                Normal
    0x80504C00 |--------------------------|             ------------
               |TTB (L2 Peripherals-B) 16k|                Normal
    0x80504800 |--------------------------|             ------------
               |TTB (L2 Peripherals-A) 16k|                Normal
    0x80504400 |--------------------------|             ------------
               |TTB (L2 Priv Periphs)  4k |                Normal
    0x80504000 |--------------------------|             ------------
               |    TTB (L1 Descriptors)  |                Normal
    0x80500000 |--------------------------|             ------------
               |           Heap           |                Normal
               |--------------------------|             ------------
               |          Stack           |                Normal
    0x80400000 |--------------------------|             ------------
               |         ZI Data          |                Normal
    0x80300000 |--------------------------|             ------------
               |         RW Data          |                Normal
    0x80200000 |--------------------------|             ------------
               |         RO Data          |                Normal
               |--------------------------|             ------------
               |         RO Code          |              USH Normal
    0x80000000 |--------------------------|             ------------
               |      Daughterboard       |                Fault
               |      HSB AXI buses       |
    0x40000000 |--------------------------|             ------------
               |      Daughterboard       |                Fault
               |  test chips peripherals  |
    0x2C002000 |--------------------------|             ------------
               |     Private Address      |            Device Memory
    0x2C000000 |--------------------------|             ------------
               |      Daughterboard       |                Fault
               |  test chips peripherals  |
    0x20000000 |--------------------------|             ------------
               |       Peripherals        |           Device Memory RW/RO
               |                          |              & Fault
    0x00000000 |--------------------------|
    */

    // L1 Cache info and restrictions about architecture of the caches (CCSIR register):
    // Write-Through support *not* available
    // Write-Back support available.
    // Read allocation support available.
    // Write allocation support available.

    // Note: You should use the Shareable attribute carefully.
    // For cores without coherency logic (such as SCU) marking a region as shareable forces the processor to not cache that region regardless of the inner cache settings.
    // Cortex-A versions of RTX use LDREX/STREX instructions relying on Local monitors. Local monitors will be used only when the region gets cached, regions that are not cached will use the Global Monitor.
    // Some Cortex-A implementations do not include Global Monitors, so wrongly setting the attribute Shareable may cause STREX to fail.

    // Recall: When the Shareable attribute is applied to a memory region that is not Write-Back, Normal memory, data held in this region is treated as Non-cacheable.
    // When SMP bit = 0, Inner WB/WA Cacheable Shareable attributes are treated as Non-cacheable.
    // When SMP bit = 1, Inner WB/WA Cacheable Shareable attributes are treated as Cacheable.

    // Following MMU configuration is expected
    // SCTLR.AFE == 1 (Simplified access permissions model - AP[2:1] define access permissions, AP[0] is an access flag)
    // SCTLR.TRE == 0 (TEX remap disabled, so memory type and attributes are described directly by bits in the descriptor)
    // Domain 0 is always the Client domain
    // Descriptors should place all memory in domain 0

    #include "<Device>.h" /* ToDo: replace '<Device>' with your device name */

    // L2 table pointers
    //-----------------------------------------------------
    #define PRIVATE_TABLE_L2_BASE_4k       (0x80504000) //Map 4k Private Address space
    #define SYNC_FLAGS_TABLE_L2_BASE_4k    (0x80504C00) //Map 4k Flag synchronization
    #define PERIPHERAL_A_TABLE_L2_BASE_64k (0x80504400) //Map 64k Peripheral #1
    #define PERIPHERAL_B_TABLE_L2_BASE_64k (0x80504800) //Map 64k Peripheral #2

    //--------------------- PERIPHERALS -------------------
    #define PERIPHERAL_A_FAULT             (0x00000000 + 0x1C000000)
    #define PERIPHERAL_B_FAULT             (0x00100000 + 0x1C000000)

    //--------------------- SYNC FLAGS --------------------
    #define FLAG_SYNC                       0xFFFFF000
    #define F_SYNC_BASE                     0xFFF00000  //1M aligned

    //Import symbols from linker
    extern uint32_t Image$$VECTORS$$Base;
    extern uint32_t Image$$RW_DATA$$Base;
    extern uint32_t Image$$ZI_DATA$$Base;
    extern uint32_t Image$$TTB$$ZI$$Base;

    static uint32_t Sect_Normal;        // outer & inner wb/wa, non-shareable, executable, rw, domain 0, base addr 0
    static uint32_t Sect_Normal_Cod;    // outer & inner wb/wa, non-shareable, executable, ro, domain 0, base addr 0
    static uint32_t Sect_Normal_RO;     // as Sect_Normal_Cod, but not executable
    static uint32_t Sect_Normal_RW;     // as Sect_Normal_Cod, but writeable and not executable
    static uint32_t Sect_Device_RO;     // device, non-shareable, non-executable, ro, domain 0, base addr 0
    static uint32_t Sect_Device_RW;     // as Sect_Device_RO, but writeable

    /* Define global descriptors */
    static uint32_t Page_L1_4k  = 0x0;  // generic
    static uint32_t Page_L1_64k = 0x0;  // generic
    static uint32_t Page_4k_Device_RW;  // shared device, not executable, rw, domain 0
    static uint32_t Page_64k_Device_RW; // shared device, not executable, rw, domain 0

    void MMU_CreateTranslationTable(void)
    {
      mmu_region_attributes_Type region;

      // Create 4GB of faulting entries
      MMU_TTSection (&Image$$TTB$$ZI$$Base, 0, 4096, DESCRIPTOR_FAULT);

      /*
       * Generate descriptors. Refer to core_ca.h to get information about attributes
       *
       */
      // Create descriptors for Vectors, RO, RW, ZI sections
      section_normal(Sect_Normal, region);
      section_normal_cod(Sect_Normal_Cod, region);
      section_normal_ro(Sect_Normal_RO, region);
      section_normal_rw(Sect_Normal_RW, region);
      // Create descriptors for peripherals
      section_Device_ro(Sect_Device_RO, region);
      section_Device_rw(Sect_Device_RW, region);
      // Create descriptors for 64k pages
      page64k_Device_rw(Page_L1_64k, Page_64k_Device_RW, region);
      // Create descriptors for 4k pages
      page4k_Device_rw(Page_L1_4k, Page_4k_Device_RW, region);

      /*
       *  Define MMU flat-map regions and attributes
       *
       */
      // Define Image
      MMU_TTSection (&Image$$TTB$$ZI$$Base, (uint32_t)&Image$$VECTORS$$Base     ,    1U, Sect_Normal_Cod);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, (uint32_t)&Image$$RW_DATA$$Base     ,    1U, Sect_Normal_RW);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, (uint32_t)&Image$$ZI_DATA$$Base     ,    1U, Sect_Normal_RW);

      // All DRAM executable, RW, cacheable - applications may choose to divide memory into RO executable
      MMU_TTSection (&Image$$TTB$$ZI$$Base, (uint32_t)&Image$$TTB$$ZI$$Base     , 2043U, Sect_Normal);

      //--------------------- PERIPHERALS -------------------
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_FLASH_BASE0    ,   64U, Sect_Device_RO);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_FLASH_BASE1    ,   64U, Sect_Device_RO);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_SRAM_BASE      ,   64U, Sect_Device_RW);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_VRAM_BASE      ,   32U, Sect_Device_RW);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_ETHERNET_BASE  ,   16U, Sect_Device_RW);
      MMU_TTSection (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_USB_BASE       ,   16U, Sect_Device_RW);

      // Create (16 * 64k)=1MB faulting entries to cover peripheral range
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, PERIPHERAL_A_FAULT                   ,   16U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, DESCRIPTOR_FAULT);
      // Define peripheral range
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_DAP_BASE        ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_SYSTEM_REG_BASE ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_SERIAL_BASE     ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_AACI_BASE       ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_MMCI_BASE       ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_KMI0_BASE       ,    2U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_UART_BASE       ,    4U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_WDT_BASE        ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_A_TABLE_L2_BASE_64k, Page_64k_Device_RW);

      // Create (16 * 64k)=1MB faulting entries to cover peripheral range
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, PERIPHERAL_B_FAULT                   ,   16U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, DESCRIPTOR_FAULT);
      // Define peripheral range
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_TIMER_BASE      ,    2U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_DVI_BASE        ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_RTC_BASE        ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_UART4_BASE      ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, Page_64k_Device_RW);
      MMU_TTPage64k(&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_CLCD_BASE       ,    1U, Page_L1_64k, (uint32_t *)PERIPHERAL_B_TABLE_L2_BASE_64k, Page_64k_Device_RW);

      // Create (256 * 4k)=1MB faulting entries to cover private address space. Needs to be marked as Device memory
      MMU_TTPage4k (&Image$$TTB$$ZI$$Base, __get_CBAR()                         ,  256U,  Page_L1_4k, (uint32_t *)PRIVATE_TABLE_L2_BASE_4k, DESCRIPTOR_FAULT);
      // Define private address space entry
      MMU_TTPage4k (&Image$$TTB$$ZI$$Base, __get_CBAR()                         ,    2U,  Page_L1_4k, (uint32_t *)PRIVATE_TABLE_L2_BASE_4k, Page_4k_Device_RW);
      // Define L2CC entry
      MMU_TTPage4k (&Image$$TTB$$ZI$$Base, <DeviceAbbreviation>_L2C_BASE        ,    1U,  Page_L1_4k, (uint32_t *)PRIVATE_TABLE_L2_BASE_4k, Page_4k_Device_RW);

      // Create (256 * 4k)=1MB faulting entries to synchronization space (Useful if some non-cacheable DMA agent is present in the SoC)
      MMU_TTPage4k (&Image$$TTB$$ZI$$Base, F_SYNC_BASE                          ,  256U, Page_L1_4k, (uint32_t *)SYNC_FLAGS_TABLE_L2_BASE_4k, DESCRIPTOR_FAULT);
      // Define synchronization space entry.
      MMU_TTPage4k (&Image$$TTB$$ZI$$Base, FLAG_SYNC                            ,    1U, Page_L1_4k, (uint32_t *)SYNC_FLAGS_TABLE_L2_BASE_4k, Page_4k_Device_RW);

      /* Set location of level 1 page table
      ; 31:14 - Translation table base addr (31:14-TTBCR.N, TTBCR.N is 0 out of reset)
      ; 13:7  - 0x0
      ; 6     - IRGN[0] 0x0 (Inner WB WA)
      ; 5     - NOS     0x0 (Non-shared)
      ; 4:3   - RGN     0x1 (Outer WB WA)
      ; 2     - IMP     0x0 (Implementation Defined)
      ; 1     - S       0x0 (Non-shared)
      ; 0     - IRGN[1] 0x1 (Inner WB WA) */
      __set_TTBR0(((uint32_t)&Image$$TTB$$ZI$$Base) | 9U);
      __ISB();

      /* Set up domain access control register
      ; We set domain 0 to Client and all other domains to No Access.
      ; All translation table entries specify domain 0 */
      __set_DACR(1);
      __ISB();
    }