CMSIS-Core (Cortex-M): MPU_Type Struct Reference

| CMSIS-Core (Cortex-M) Version 5.1.2 CMSIS-Core support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Data Fields
MPU_Type Struct Reference
MPU Functions for Armv7-M

Structure type to access the Memory Protection Unit (MPU).

## Data Fields
__IM uint32_t | TYPE
| Offset: 0x000 (R/ ) MPU Type Register. More...
__IOM uint32_t | CTRL
| Offset: 0x004 (R/W) MPU Control Register. More...
__IOM uint32_t | RNR
| Offset: 0x008 (R/W) MPU Region RNRber Register. More...
__IOM uint32_t | RBAR
| Offset: 0x00C (R/W) MPU Region Base Address Register. More...
__IOM uint32_t | RASR
| Offset: 0x010 (R/W) MPU Region Attribute and Size Register. More...
__IOM uint32_t | RBAR_A1
| Offset: 0x014 (R/W) MPU Alias 1 Region Base Address Register. More...
__IOM uint32_t | RASR_A1
| Offset: 0x018 (R/W) MPU Alias 1 Region Attribute and Size Register. More...
__IOM uint32_t | RBAR_A2
| Offset: 0x01C (R/W) MPU Alias 2 Region Base Address Register. More...
__IOM uint32_t | RASR_A2
| Offset: 0x020 (R/W) MPU Alias 2 Region Attribute and Size Register. More...
__IOM uint32_t | RBAR_A3
| Offset: 0x024 (R/W) MPU Alias 3 Region Base Address Register. More...
__IOM uint32_t | RASR_A3
| Offset: 0x028 (R/W) MPU Alias 3 Region Attribute and Size Register. More...

## Field Documentation

MPU_Type::CTRL

Enables the MPU, and when the MPU is enabled, controls whether the default memory map is enabled as a background region for privileged accesses, and whether the MPU is enabled for HardFaults, NMIs, and exception handlers when FAULTMASK is set to 1.

Bits | Name | Function
--- | --- | ---
[31:3] | - | Reserved.
[2] | PRIVDEFENA | 0 - Disables the default memory map. 1 - Enables the default memory map as a background region for privileged access.
[1] | HFNMIENA | 0 - Disables the MPU for exception handlers. 1 - Use the MPU for memory accesses by exception handlers.
[0] | ENABLE | 0 - The MPU is disabled. 1 - The MPU is enabled.

MPU_Type::RASR

Defines the size and access behavior of the region identified by MPU_RNR, and enables that region.

Bits | Name | Function
--- | --- | ---
[31:29] | - | Reserved.
[28] | XN | Execute Never.
[27] | - | Reserved.
[26:24] | AP | Access Permissions, see ARM_MPU_AP_xxx.
[23:22] | - | Reserved.
[21:19] | TEX | Type Extension.
[18] | S | Shareable.
[17] | C | Cacheable.
[16] | B | Bufferable.
[15:8] | SRD | Subregion Disable. For regions of 256 bytes or larger, each bit of this field controls whether one of the eight equal subregions is enabled (0) or disabled (1).
[7:6] | - | Reserved.
[5:1] | SIZE | Indicates the region size. The region size, in bytes, is 2(SIZE+1). SIZE field values less than 4 are reserved, because the smallest supported region size is 32 bytes.
[0] | ENABLE | 0 - This region is disabled. 1 - This region is enabled.

MPU_Type::RASR_A1

Alias for MPU_Type::RASR.

MPU_Type::RASR_A2

Alias for MPU_Type::RASR.

MPU_Type::RASR_A3

Alias for MPU_Type::RASR.

MPU_Type::RBAR

Holds the base address of the region identified by MPU_RNR. On a write, can also be used to update the base address of a specified region, in the range 0 to 15, updating MPU_RNR with the new region number.

Bits | Name | Function
--- | --- | ---
[31:5] | ADDR | Base address of the region.
[4] | VALID | 1 - Update MPU_Type::RNR to the value obtained by zero extending the REGION value specified in this write, and apply the base address update to this region.
[3:0] | REGION | On writes, can specify the number of the region to update, see VALID field description.

MPU_Type::RBAR_A1

Alias for MPU_Type::RBAR.

MPU_Type::RBAR_A2

Alias for MPU_Type::RBAR.

MPU_Type::RBAR_A3

Alias for MPU_Type::RBAR.

MPU_Type::RNR

Selects the region currently accessed by MPU_Type::RBAR and MPU_Type::RASR.

Bits | Name | Function
--- | --- | ---
[31:8] | - | Reserved.
[7:0] | REGION | Indicates the memory region accessed.

MPU_Type::TYPE

The MPU Type Register indicates how many regions the MPU support. Software can use it to determine if the processor implements an MPU.

Bits | Name | Function
--- | --- | ---
[31:24] | - | Reserved.
[23:16] | IREGION | Instruction region. RAZ. Armv7-M only supports a unified MPU.
[15:8] | DREGION | Number of regions supported by the MPU. If this field reads-as-zero the processor does not implement an MPU.
[7:1] | - | Reserved.
[0] | SEPARATE | Indicates support for separate instruction and data address maps. RAZ. Armv7-M only supports a unified MPU.