CMSIS-DAP: DAP_SWD_Configure

| CMSIS-DAP Version 2.0.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_SWD_Configure
SWD Commands

Configure SWD Protocol. More...

Configure SWD Protocol.

The DAP_SWD_Configure Command sets the SWD protocol configuration. For more information about the SWD protocol refer to the Arm Debug Interface v5 - Interface Specification.

DAP_SWD_Configure Command:

| BYTE | BYTE *********|
> 0x13 | Configuration |
|******|***************|

- Configuration: Contains information about SWD specific features
  - Bit 1 .. 0: Turnaround clock period of the SWD device (should be identical with the WCR [Write Control Register] value of the target): 0 = 1 clock cycle (default), 1 = 2 clock cycles, 2 = 3 clock cycles, 3 = 4 clock cycles.
  - Bit 2: DataPhase: 0 = Do not generate Data Phase on WAIT/FAULT (default), 1 = Always generate Data Phase (also on WAIT/FAULT; Required for Sticky Overrun behavior).

DAP_SWD_Configure Response:

| BYTE | BYTE **|
< 0x13 | Status |
|******|********|

- Status: Response Status