CMSIS-Driver: NAND Control Codes

| CMSIS-Driver Version 2.6.0 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content
NAND Control Codes
NAND Interface

Many parameters of the NAND driver are configured using the ARM_NAND_Control function. More...

## Content
| NAND Mode Controls
| Specify operation modes of the NAND interface.
| NAND Bus Modes
| Specify bus mode of the NAND interface.
| NAND Data Bus Width
| Specify data bus width of the NAND interface.
| NAND Driver Strength
| Specify driver strength of the NAND interface.

## Description

Many parameters of the NAND driver are configured using the ARM_NAND_Control function.

Refer to the function ARM_NAND_Control for further details.