CMSIS-Pack: System Description File (*.SDF) Format

| CMSIS-Pack Version 1.5.0 Delivery Mechanism for Software Packs

- Main Page
- Usage and Description

All Pages
System Description File (*.SDF) Format

An SDF file enables the silicon provider to describe more complex debug topologies than with a Debug Description in a tool agnostic way. Multiple debug and access ports and the setup of the different debug/trace components can be described consistently. Also, mandatory settings for a debugger can be described, such as trace signal delay settings, availability/usability of certain reset methods or timings, etc. This information is used by the debugger to access the right components that are requested by the user or application. The SDF format provides the XML elements for defining the debug system view of a device. These are "expert" settings that cannot be specified in a PDSC file.

Note
  SDF files are referenced in a PDSC file via the `<debugconfig>` element.

Example CMSIS System Description File (*.SDF)

<?xml version="1.0" encoding="utf-8" standalone="no"?>
<system_description version="2.0">
<debug_and_trace_config>
<!-- Not filled at the moment -->
<!-- Means using defaults in this area -->
</debug_and_trace_config>
<platform>
<!-- Description of the scanchain -->
<scanchain>
<!-- ARM Cortex-M0APP -->
<dap name="ARMCS-DP_CM0APP" type="ARMCS-DP" irLength="4" protocol="JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x0BA01477</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM0APP_AHB-AP" type="CSMEMAP"> <!-- Cortex-M0APP AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
<!-- Cortex-M0APP AHB-AP Components -->
<device name="CM0APP_CPU" type="Cortex-M0">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE000E000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_DWT" type="CSDWT">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0001000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_FPB" type="CSFPB">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0002000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
</dap>
<!-- ARM Cortex-M4 -->
<dap name="ARMCS-DP_CM4" type="ARMCS-DP" irLength="4" protocol="SWD:JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x4BA00477</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM4_AHB-AP" type="CSMEMAP"> <!-- Cortex-M4 AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
<!-- Cortex-M4 AHB-AP Components -->
<device name="CM4_CPU" type="Cortex-M4">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE000E000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_DWT" type="CSDWT">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0001000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_FPB" type="CSFPB">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0002000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ITM" type="CSITM">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0000000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_TPIU" type="CSTPIU">
<device_info_items>
<device_info_item name="ARCHITECTURE" >V7-M</device_info_item>
<device_info_item name="SUPPORTED_FORMATTER_MODES">CONTINUOUS</device_info_item>
<device_info_item name="SUPPORTED_PORT_SIZES" >1;2;4</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0040000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ETM" type="CSETM">
<device_info_items>
<device_info_item name="VERSION">3.5</device_info_item>
<device_info_item name="SUPPORTS_CYCLE_ACCURATE">true</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0041000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ETB" type="CSETB">
<device_info_items>
<device_info_item name="MEM_WIDTH" >32</device_info_item>
<device_info_item name="RAM_SIZE_BYTES">0x4000</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0042000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
</dap>
</scanchain>
<topology>
<!-- Trace Links -->
<!-- Core Trace - Cortex-M4 -->
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_DWT"/>
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_ITM"/>
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_ETM"/>
<topology_link type="ATB" master="CM4_ETM" slave="CM4_TPIU" slave_interface="0"/>
<topology_link type="ATB" master="CM4_ITM" slave="CM4_TPIU" slave_interface="1"/>
<!-- Trace - Cortex-M4 ETB (Direct Connection ETM -> ETB) -->
<topology_link type="ATB" master="CM4_ETM" slave="CM4_ETB"/>
</topology>
</platform>
</system_description>

# SDF top level structure

The XML schema file sdf_schema.xsd defines the sections used in a *.SDF file. The current sdf_schema.xsd can be found under the ARM.CMSIS.*.Pack in the .\CMSIS\Utilities-directory.

# /system_description

Parents | Element Chain
--- | ---
root | description root point for SDF
Attributes | Description | Type | Use
schemaVersion | Version of sdf_schema.xsd the description is compatible with | xs:decimal | required
Child Elements | Description | Type | Occurrence
/system_description/debug_and_trace_config | Description how to configure debug and trace. | complexType | 1..1
/system_description/platform | Overall platform description. | complexType | 1..1

# /system_description/debug_and_trace_config

Describes the recommended debug and trace configuration for the device.

Parents | Element Chain
--- | ---
system_description | /system_description
Child Elements | Description | Type | Occurrence
/system_description/debug_and_trace_config/debug | Describes the debug connection configuration | complexType | 0..1
/system_description/debug_and_trace_config/trace | Describes the trace configuration | complexType | 0..1

# /system_description/debug_and_trace_config/debug

Describes the recommended debug configuration for the device.

Parents | Element Chain
--- | ---
debug_and_trace_config | /system_description/debug_and_trace_config
Child Elements | Description | Type | Occurrence
/system_description/.../config_item | Describes a configuration item attribute/value pair | xs:string | 0..*

For a list of applicable configuration items, refer to config_item.

# /system_description/.../config_item

A config_item can appear in various SDF elements. This group contains individual configuration items.

Parents | Element Chain
--- | ---
debug | /system_description/debug_and_trace_config/debug
trace_capture | /system_description/debug_and_trace_config/trace/trace_capture
config_items | /system_description/platform/scanchain/../config_items
Attributes | Description | Type | Use
name | Name of the configuration item. | xs:string | required

## Debug element

The config_items applicable to the debug element are the following:

Item | Description
--- | ---
TRSTOnConnect | Debugger should perform TAP reset on connect (True/False) - Default Value:True
SRSTOnConnect | Debugger should perform a System reset on connect (True/False) - Default Value:False
AllowTRST | Allow the Debugger to perform TAP reset (True/False) - Default Value:True
DoSoftTRST | Debugger should perform a Soft Reset (True/False) - Default Value:True
TRSTHoldTime | TAP reset hold time in milliseconds - Default Value:10
TRSTPostResetTime | Delay after TAP reset before next operation - Default Value:10
ResetHoldTime | Time in milliseconds that the target is held in a hardware reset state - Default Value:100
PostResetDelay | Time in milliseconds that the target will wait after reset is released before attempting any other debugging operations - Default Value:10
Linked_SRST_TRST | Target hardware has System Reset and TAP reset physically linked (True/False) - Default Value:False

## Device element

The config_items applicable to the device element are the following (only applicable for devices that are child elements of another device or DAP):

Item | Description | Use
--- | --- | ---
CORESIGHT_BASE_ADDRESS | the 4K aligned base address of a CoreSight device | Required
CORESIGHT_AP_INDEX | the access port index of the device | Required

## Trace element

The config_items applicable to the trace element are the following:

1. Parallel trace capture device configuration items ("type" = "parallel"). These "config_items" enable you to configure delays on the trace lines by a specified amount of time relative to the trace capture device defaults. These delays are used to allow for variations in target hardware. These configuration items have default values if not present.

   Item | Description | Default
   --- | --- | ---
   CLOCK_EDGE | Set to 0 or 1 to specify the clock edge on which to capture data | 1
   DELAY_TRACE_CLOCK | Adjust the sampling point for the trace clock by the specified number of picoseconds | 0
   DELAY_TRACE_SIGNAL_1 to DELAY_TRACE_SIGNAL_n | Adjust the sampling point for parallel trace signal 'n' by the specified number of picoseconds | 0

2. High-speed serial trace configuration items ("type"="HSSTP"). These configuration items do not have any default values. If they are not present in the SDF file then HSSTP trace is not supported by the target.

   Item | Description
   --- | ---
   HSSTP_LANES | The number of lanes (1-6)
   HSSTP_SPEED | The HSSTP link speed (HSSTP_2_5Gbps, , HSSTP_3_0Gbps, HSSTP_3_125Gbps, HSSTP_4_25Gbps, HSSTP_5_0Gbps, HSSTP_6_0Gbps, HSSTP_6_25Gbps, HSSTP_8_0Gbps, HSSTP_10_0Gbps, HSSTP_10_3125Gbps, HSSTP_12_0Gbps, HSSTP_12_5Gbps, HSSTP_SETM_1_5Gbps, HSSTP_SETM_3_0Gbps, HSSTP_SETM_6_0Gbps)
   HSSTP_PROTOCOL | The HSSTP protocol (HSSTP_PROTOCOL_ARM_HSSTP, HSSTP_PROTOCOL_8_BIT_SETM, HSSTP_PROTOCOL_16_BIT_SETM, HSSTP_PROTOCOL_32_BIT_SETM)
   HSSTP_NDALT | Reverse byte bit-ordering (HSSTP_NDALT_Disabled/HSSTP_NDALT_Enabled)
   HSSTP_CONNECTOR | The physical connector type (HSSTP_CONNECTOR_HSSTP/HSSTP_CONNECTOR_SMA)
   HSSTP_RX_EQUALIZATION | The RX equalization type (RX_EQUALIZATION_DFE/RX_EQUALIZATION_LPM)
   HSSTP_CRC | The type of CRC to use (HSSTP_CRC_Enabled, HSSTP_CRC_Disabled, HSSTP_CRC_Reversed, HSSTP_CRC_Ignored)

   Example

...
<device name="CM4_ETM" type="CSETM">
<device_info_items>
<device_info_item name="VERSION">3.5</device_info_item>
<device_info_item name="SUPPORTS_CYCLE_ACCURATE">true</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0041000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
...

# /system_description/debug_and_trace_config/trace

Describes the recommended trace configuration for the device.

Parents | Element Chain
--- | ---
debug_and_trace_config | /system_description/debug_and_trace_config
Child Elements | Description | Type | Occurrence
/system_description/debug_and_trace_config/trace/trace_capture | Describes the trace capture device | complexType | 0..*

# /system_description/debug_and_trace_config/trace/trace_capture

Describes settings for the trace capture device.

Parents | Element Chain
--- | ---
trace | /system_description/debug_and_trace_config/trace
Child Elements | Description | Type | Occurrence
/system_description/.../config_item | Describes a configuration item attribute/value pair | complexType | 0..*
Attributes | Description | Type | Use
type | Trace capture type: for example parallel or HSSTP. | xs:string | required

# /system_description/platform

Describes the platform configuration (scanchain, topology and cluster arrangement).

Parents | Element Chain
--- | ---
system_description | /system_description
Child Elements | Description | Type | Occurrence
/system_description/platform/scanchain | Lists all DAPs/Devices in the order that they appear on the scanchain (Note - order is reverse to DAP references in PDSC files). The first device in the scanchain is one closest to target's TDI pin. | complexType | 0..*
/system_description/platform/topology | Describes the system topology | complexType | 0..1
/system_description/platform/clusters | Describes the cluster arrangement | complexType | 0..1

# /system_description/platform/scanchain

Lists all DAPs/devices in the order that they appear on the scanchain.

Note
  The order is reverse to the DAP references in PDSC files. The first device in the scanchain is the one closest to the target's TDI pin.

Parents | Element Chain
--- | ---
platform | /system_description/platform
Child Elements | Description | Type | Occurrence
/system_description/platform/scanchain/dap | Describes a DAP and a list of devices associated with that DAP. | complexType | 0..*
/system_description/platform/scanchain/device | Describes a single device on the scan chain. | complexType | 0..*

Example:

...
<!-- Description of the scanchain -->
<scanchain>
<!-- ARM Cortex-M0APP -->
<dap name="ARMCS-DP_CM0APP" type="ARMCS-DP" irLength="4" protocol="JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x0BA01477</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM0APP_AHB-AP" type="CSMEMAP"> <!-- Cortex-M0APP AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
<!-- Cortex-M0APP AHB-AP Components -->
<device name="CM0APP_CPU" type="Cortex-M0">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE000E000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_DWT" type="CSDWT">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0001000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_FPB" type="CSFPB">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0002000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
</dap>
<!-- ARM Cortex-M4 -->
<dap name="ARMCS-DP_CM4" type="ARMCS-DP" irLength="4" protocol="SWD:JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x4BA00477</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM4_AHB-AP" type="CSMEMAP"> <!-- Cortex-M4 AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
<!-- Cortex-M4 AHB-AP Components -->
<device name="CM4_CPU" type="Cortex-M4">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE000E000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_DWT" type="CSDWT">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0001000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_FPB" type="CSFPB">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0002000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ITM" type="CSITM">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0000000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_TPIU" type="CSTPIU">
<device_info_items>
<device_info_item name="ARCHITECTURE" >V7-M</device_info_item>
<device_info_item name="SUPPORTED_FORMATTER_MODES">CONTINUOUS</device_info_item>
<device_info_item name="SUPPORTED_PORT_SIZES" >1;2;4</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0040000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ETM" type="CSETM">
<device_info_items>
<device_info_item name="VERSION">3.5</device_info_item>
<device_info_item name="SUPPORTS_CYCLE_ACCURATE">true</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0041000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM4_ETB" type="CSETB">
<device_info_items>
<device_info_item name="MEM_WIDTH" >32</device_info_item>
<device_info_item name="RAM_SIZE_BYTES">0x4000</device_info_item>
</device_info_items>
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0042000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
</dap>
</scanchain>
...

# /system_description/platform/scanchain/dap

Describes a DAP and a list of devices associated with that DAP.

Parents | Element Chain
--- | ---
scanchain | /system_description/platform/scanchain
Child Elements | Description | Type | Occurrence
/system_description/platform/scanchain/device | List of devices associated with this DAP. | complexType | 0..*
/system_description/platform/scanchain/../../device_info_items | Contains implementation details for the DAP. Applicable items for a DAP are "JTAG_IDCODE" (the JTAG ID code for the DAP) or "DPIDR" (the Debug Port Identification Register contents). | complexType | 0..*
/system_description/platform/scanchain/../../config_items | Configuration items specific to a DAP type. | complexType | 0..*
Attributes | Description | Type | Use
name | Unique name of the DAP. | xs:string | required
type | Specifies the type of the DAP (e.g. ARMCS-DP). | xs:string | required
irLength | Specifies the IR length of the DAP (default value: 4). | xs:string | optional
protocol | Colon delimited list of protocols via which the DAP can be use. Possible values are SWD, JTAG, and cJTAG. | xs:string | optional
targetsel | Specifies the SW-DPv2 TARGETSEL register value that selects this DAP in a serial-wire debug multi-drop system. | xs:string | optional

Example:

<system_description version="2.0">
<debug_and_trace_config>
<!-- Not filled at the moment -->
<!-- Means using defaults in this area -->
</debug_and_trace_config>
<platform>
<!-- Description of the scanchain -->
<scanchain>
<!-- ARM Cortex-M0APP -->
<dap name="ARMCS-DP_CM0APP" type="ARMCS-DP" irLength="4" protocol="JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x0BA01477</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM0APP_AHB-AP" type="CSMEMAP"> <!-- Cortex-M0APP AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
<!-- Cortex-M0APP AHB-AP Components -->
<device name="CM0APP_CPU" type="Cortex-M0">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE000E000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_DWT" type="CSDWT">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0001000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
<device name="CM0APP_FPB" type="CSFPB">
<config_items>
<config_item name="CORESIGHT_BASE_ADDRESS">0xE0002000</config_item>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
</device>
</dap>
...
</system_description>

# /system_description/platform/scanchain/device

Parents | Element Chain
--- | ---
scanchain | /system_description/platform/scanchain
dap | /system_description/platform/scanchain/dap
Child Elements | Description | Type | Occurrence
/system_description/platform/scanchain/device | Describes a single nested device associated with this device. | complexType | 0..*
/system_description/platform/scanchain/../../device_info_items | Describes a sequence of device information items. | complexType | 0..*
/system_description/platform/scanchain/../../config_items | Configuration items specific to this device. | complexType | 0..*
Attributes | Description | Type | Use
name | Unique name of the device. | xs:string | required
type | Specifies the device type (see below). | xs:string | required
irLength | Specifies the IR length of the device (default value: 4). | xs:string | optional

Depending on the context, a device type can be one of the following types:

1. A core device, where the type is usually specified as "Cortex-xx" (such as Cortex-A72,Cortex-M0+, Cortex-R5). It can also be a vendor-specific core type, or an older JTAG ARM core. Current cores are:
   "Cortex-A5", "Cortex-A7", "Cortex-A8", "Cortex-A9", "Cortex-A12", "Cortex-A15", "Cortex-A17", "Cortex-A32", "Cortex-A35", "Cortex-A53", "Cortex-A57", "Cortex-A72", "Cortex-A73", "Cortex-M0", "Cortex-M0+", "Cortex-M0+_JTAG-AP", "Cortex-M1", "Cortex-M23", "Cortex-M3", "Cortex-M33", "Cortex-M3_JTAG-AP", "Cortex-M4", "Cortex-M7", "Cortex-R4", "Cortex-R5", "Cortex-R7", "Cortex-R8", "Cortex-R52", "SC000", "SC100D", "SC200D", "SC300", "ThunderX", "ThunderX-r2", "ARMV8MBL", "ARMV8MML", "88FR101", "88FR111", "88FR331", "88SV581x-v7_PJ4", "88SV581x-v7_PJ4_TZ", "ARM1136JF-S", "ARM1136JF-S_JTAG-AP", "ARM1156T2F-S", "ARM1156T2F-S_JTAG-AP", "ARM1176JZF-S", "ARM1176JZF-S_JTAG-AP", "ARM11MPCore", "ARM11MPCore_JTAG-AP", "ARM710T", "ARM720T", "ARM720T_r4", "ARM740T", "ARM7EJ-S", "ARM7EJ-S_JTAG-AP", "ARM7TDMI", "ARM7TDMI_JTAG-AP", "ARM7TDMI_r4", "ARM7TDMI_r4_JTAG-AP", "ARM920T", "ARM922T", "ARM925T", "ARM926EJ-S", "ARM926EJ-S_JTAG-AP", "ARM940T", "ARM946E-S", "ARM946E-S_JTAG-AP", "ARM966E-S", "ARM966E-S_JTAG-AP", "ARM968E-S", "ARM968E-S_JTAG-AP", "ARM968E-Srd", "ARM996HS", "ARM9E-S", "ARM9EJ-S", "ARM9EJ-S_JTAG-AP", "ARM9TDMI", "V7A-Generic", "V8-Generic", "V8M-Generic", "V8R-Generic", "V8_1-Generic", "V8_2-Generic".
2. An Access Port (AP) type such as "CSAUTHAP", "CSJTAGAP" or "CSMEMAP".
3. A CoreSight device type that can be one of "CSCTI", "CSETM", "CSITM", "CSMTB", "CSPMU", "CSPTM", "CSTFunnel", "CSTMC", "CSTPIU","CSSTM", "CSSWO", "CSELA", "CSATBReplicator", "CSGPR", "CSETB", "CSDWT", "CSETB", "CSTSGEN", "CSHTM", "CSFPB"
4. A JTAG device, which is directly on the scanchain (e.g. ARM11).

Example:

<system_description version="2.0">
<debug_and_trace_config>
<!-- Not filled at the moment -->
<!-- Means using defaults in this area -->
</debug_and_trace_config>
<platform>
<!-- Description of the scanchain -->
<scanchain>
<device name="My Custom TAP" type="Other" irLength="5">
<!-- JTAG-TAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x04560014</device_info_item>
</device_info_items>
</device>
...
</system_description>

# /system_description/platform/scanchain/../../config_items

The configuration items are specific to the device type or DAP. Refer to /system_description/.../config_item for a list of applicable device information items and a code example.

Parents | Element Chain
--- | ---
device | /system_description/platform/../device
dap | /system_description/platform/scanchain/dap
Child Elements | Description | Type | Occurrence
/system_description/.../config_item | Describes a configuration item. | complexType | 0..*

# /system_description/platform/scanchain/../../device_info_items

The device information items are specific to the type of device or DAP and describe implementation specific details. Refer to /system_description/platform/scanchain/../../device_info_items/device_info_item for a list of applicable device information items and a code example.

Parents | Element Chain
--- | ---
device | /system_description/platform/../device
dap | /system_description/platform/scanchain/dap
Child Elements | Description | Type | Occurrence
/system_description/platform/scanchain/../../device_info_items/device_info_item | Describes a sequence of device information items. | xs:string | 0..*

# /system_description/platform/scanchain/../../device_info_items/device_info_item

Describes implementation specific details of the specified device or DAP.

Parents | Element Chain
--- | ---
device_info_items | /system_description/platform/../../device_info_items
Attributes | Description | Type | Use
name | Unique name for the device information item. | xs:string | required

The following device information items are applicable for each type of "device":

Device | Device Information Item | Description
--- | --- | ---
CSMEMAP | AP_TYPE | Access port type is one of AHB-AP, APB-AP-M, APB-AP and AXI-AP
| ROM_TABLE_BASE_ADDRESS | The ROM table base address (in hex)
CSETM | VERSION | The ETM Version (e.g. 4.0 - required)
| SUPPORTS_CONTEXT_IDS | Supports Context ID Tracing (True/False - Default Value:False)
| SUPPORTS_VIRTUAL_CONTEXT_IDS | Supports Virtual Context ID Tracing (True/False - Default Value:False)
| SUPPORTS_CYCLE_ACCURATE | Supports Cycle Accurate Trace (True/False - Default Value:False)
| SUPPORTS_DATA_VALUE_TRACE | Supports Data Value Trace (True/False - Default Value:False)
| SUPPORTS_DATA_ADDRESS_TRACE | Supports Data Address Trace (True/False - Default Value:False)
| SUPPORTS_DATA_ONLY_MODE | Supports Data Only Trace Mode (True/False - Default Value:False)
| SUPPORTS_TIMESTAMPS | Supports Timestamps(True/False - Default Value:False)
| SUPPORTS_TRACE_RANGES | Supports Trace Ranges (True/False - Default Value:False)
| SUPPORTS_BRANCH_BROADCAST | Supports Branch Broadcasting (True/False - Default Value:False)
| SUPPORTS_CONDITIONAL_INSTRUCTIONS | Supports tracing conditional non-branch instruction (True/False - Default Value:False)
| SUPPORTS_Q_ELEMENTS | Supports Q Elements (True/False - Default Value:False)
CSMTB | RAM_SIZE_BYTES | MTB SRAM buffer size in bytes
| SUPPORTS_USER_PRIV | User/Privileged support present
CSTPM | VERSION | The PTM Version (eg 1.1) - Required
| SUPPORTS_VMID | VMID Tracing support (True/False - Default Value:False)
| SUPPORTS_CONTEXT_IDS | Context ID Tracing support (True/False - Default Value:False)
| SUPPORTS_RETURN_STACK | Return stack support (True/False - Default Value:False)
| SUPPORTS_CYCLE_ACCURATE | Cycle Accurate trace support (True/False - Default Value:False)
| SUPPORTS_BRANCH_BROADCAST | Supports Branch Broadcasting (True/False - Default Value:False)
| SUPPORTS_TIMESTAMPS | Supports Timestamping (True/False - Default Value:False)
| SUPPORTS_FIFOFULL | Supports FIFOFULL (True/False - Default Value:False)
CSTMC | CONFIG_TYPE | The TMC device configuration can be one of (ETR, ETF or ETB) - required
| RAM_SIZE_BYTES | The SRAM memory size used in ETF and ETR configurations (512 Bytes to 4 GiB) - Default: 512 Bytes
CSTPIU | SUPPORTED_PORT_SIZES | Semicolon separated list of supported port sizes (in bits) - required
| ARCHITECTURE | The TPIU variant is one of (Coresight, TPIU-Lite, V7-M or V8-M) - Required

Example:

<system_description version="2.0">
...
<platform>
<!-- Description of the scanchain -->
<scanchain>
<!-- ARM Cortex-M0APP -->
<dap name="ARMCS-DP_CM0APP" type="ARMCS-DP" irLength="4" protocol="JTAG">
<!-- CoreSight DAP Info -->
<device_info_items>
<device_info_item name="JTAG_IDCODE">0x00000000</device_info_item>
</device_info_items>
<!-- Access Ports -->
<device name="CM0APP_AHB-AP" type="CSMEMAP"> <!-- Cortex-M0APP AHB-AP -->
<config_items>
<config_item name="CORESIGHT_AP_INDEX">0</config_item>
</config_items>
<device_info_items>
<device_info_item name="AP_TYPE">AHB-AP</device_info_item>
<device_info_item name="ROM_TABLE_BASE_ADDRESS">0xE00FF000</device_info_item>
</device_info_items>
</device>
...

# /system_description/platform/topology

Describes the system topology.

Parents | Element Chain
--- | ---
platform | /system_description/platform
Child Elements | Description | Type | Occurrence
/system_description/platform/topology/topology_link | Describes how CoreSight devices and cores are connected. | complexType | 0..*

Example:

<system_description version="2.0">
<debug_and_trace_config>
</debug_and_trace_config>
<platform>
...
<topology>
<!-- Trace Links -->
<!-- Core Trace - Cortex-M4 -->
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_DWT"/>
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_ITM"/>
<topology_link type="CoreTrace" master="CM4_CPU" slave="CM4_ETM"/>
<topology_link type="ATB" master="CM4_ETM" slave="CM4_TPIU" slave_interface="0"/>
<topology_link type="ATB" master="CM4_ITM" slave="CM4_TPIU" slave_interface="1"/>
<!-- Trace - Cortex-M4 ETB (Direct Connection ETM -> ETB) -->
<topology_link type="ATB" master="CM4_ETM" slave="CM4_ETB"/>
</topology>
</platform>
</system_description>

# /system_description/platform/topology/topology_link

Describes how CoreSight devices and cores are connected.

Parents | Element Chain
--- | ---
topology | /system_description/platform/topology
Attributes | Description | Type | Use
name | Unique name for the link. | xs:string | optional
type | Specifies the link type. Can be on of the following: ATB, CoreTrace, or CTITrigger. | xs:string | required
master | Unique name of the master device in the link. | xs:string | required
slave | Unique name of the slave device in the link. | xs:string | required
mater_interface | Specifies the mater interface number. | xs:string | optional
slave_interface | Specifies the slave interface number. | xs:string | optional
trigger | Specifies the trigger number. | xs:string | optional

Example:

A complete set of links for a Cortex-A7 implementation with ETM and TPIU might look like this:

master="Cortex-A7_0" slave="CSCTI_6" trigger="7" type="CTITrigger"
master="CSETM_0" slave="CSCTI_6" trigger="6" type="CTITrigger"
master="Cortex-A7_0" slave="CSETM_0" type="CoreTrace"
master="CSETM_0" slave="CSTFunnel_2" slave_interface="0" type="ATB"
master="CSTFunnel_2" slave="CSTFunnel_0" slave_interface="1" type="ATB"
master="CSTFunnel_0" slave="CSTMC_0" type="ATB"
master="CSTMC_0" slave="CSTPIU" type="ATB"

# /system_description/platform/clusters

Describes the cluster arrangement.

Parents | Element Chain
--- | ---
platform | /system_description/platform
Child Elements | Description | Type | Occurrence
/system_description/platform/clusters/cluster | Lists the devices that make up the cluster and a unique name for the cluster. | complexType | 0..*

# /system_description/platform/clusters/cluster

Lists the devices that make up the cluster.

Parents | Element Chain
--- | ---
clusters | /system_description/platform/clusters
Attributes | Description | Type | Use
name | Unique name for the cluster (for example Cortex-A15_SMP_0). | xs:string | required
devices | Colon separated list of named devices in the cluster, for example "Cortex-A15_0:Cortex-A15_1:Cortex-A15_2:Cortex-A15_3". | xs:string | required