Back to Release page
# Release Notes for STM32F072B-Discovery Applications Copyright 2016 STMicroelectronics
## Update History ### V1.11.0 / 12-September-2019 Main Changes Update for compatibility with FreeRTOS v10.0.1_20190329 Update for compatibility with TouchSensing v2.2.4 Update for compatibility with USB Device v2.5.3 Update stm32f0xx_hal_conf.h files : Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Add reference to HAL EXTI driver Add registers callbacks defines ### V1.9.0 / 25-August-2017 Main Changes Maintenance release. Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Add a note in DFU example readme : "How to instal Dfuse demo under Window 8.1". Align stm32f0xx_hal_conf.h with latest template defined in HAL. Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Remove Cortex-M3/M4 specific defines and macros in FreeRTOSConfig.h from all FreeRTOS based applications. ### V1.8.0 / 07-April-2017 Main Changes Maintenance release Update stm32f0xx_hal_conf.h files : Compliancy with MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). Add definition of USE_SPI_CRC Update FreeRTOS_ThreadCreation example to be aligned with latest reference code. ### V1.7.0 / 04-November-2016 Main Changes Maintenance release Change of HAL API for TIM : add AutoReloadPreload capability in TIM handler. Impacts in FreeRTOS examples. Updated DFU_Standalone and HID_Standalone examples to fix issue related configuration of PIN ; Pin is now set to GPIO_MODE_INPUT ### V1.6.0 / 27-May-2016 Main Changes Maintenance release. Updated system_stm32f0xx.c files: Added APBPrescTable definition. Updated HEAP size for FreeRTOS applications (updates in FreeRTOSConfig.h). ### V1.5.0 / 29-January-2016 Main Changes Maintenance release. Add support of System Workbench for STM32 (SW4STM32) toolchain. Updated GPIO Output Speed literals naming to ensure HAL full compatibility. Added TouchSensing/TouchSensing_Linear_IT application, using the STMTouch driver with 1 linear sensor in Interrupt mode. Corrected EXTI line used in USB_Device/HID_Standalone project. Updated system_stm32f0xx.c files: Removed __IO or __I on constant table declaration. Added HSI48_VALUE definition. Updated stm32f0xx_hal_conf.h files: Set HSE_STARTUP_TIMEOUT value to 100ms instead of 5000ms Updated “Liberty” License with the new license “Ultimate Liberty”. ### V1.3.0 / 26-June-2015 Main Changes Adapt existing projects to use FreeRTOS V8.2.1. Update USB application projects. Fix known defects and several enhancements implementation. Complete HAL API alignment (renaming). ### V1.2.0 / 05-Dec-2014 Main Changes Update for compatibility with: FatFS R0.10b_STM32Cube_20141120 USB_device V2.3.0 FreeRTOS V8.1.2_20141204 ### V1.0.0 / 18-Juin-2014 Main Changes First official release. ## License This software component is licensed by ST under Ultimate Liberty license SLA0044, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/SLA0044 For complete documentation on STM32 Microcontrollers visit www.st.com/STM32