/**
  @page GPIO_InfiniteLedToggling_Init GPIO example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    Examples_LL/GPIO/GPIO_InfiniteLedToggling_Init/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the GPIO example.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright (c) 2016 STMicroelectronics.
  * All rights reserved.</center></h2>
  *
  * This software component is licensed by ST under BSD 3-Clause license,
  * the "License"; You may not use this file except in compliance with the
  * License. You may obtain a copy of the License at:
  *                        opensource.org/licenses/BSD-3-Clause
  *
  ******************************************************************************
  @endverbatim

@par Example Description

How to configure and use GPIOs to toggle the on-board user LEDs 
every 250 ms. This example is based on the STM32F1xx LL API. The peripheral 
is initialized with LL initialization function to demonstrate LL init usage.

PA.05 IO (configured in output pushpull mode) toggles in a forever loop.
On STM32F103RB-Nucleo board this IO is connected to LED2.

In this example, HCLK is configured at 72 MHz.


@par Directory contents 

  - GPIO/GPIO_InfiniteLedToggling_Init/Inc/stm32f1xx_it.h          Interrupt handlers header file
  - GPIO/GPIO_InfiniteLedToggling_Init/Inc/main.h                  Header for main.c module
  - GPIO/GPIO_InfiniteLedToggling_Init/Inc/stm32_assert.h          Template file to include assert_failed function
  - GPIO/GPIO_InfiniteLedToggling_Init/Src/stm32f1xx_it.c          Interrupt handlers
  - GPIO/GPIO_InfiniteLedToggling_Init/Src/main.c                  Main program
  - GPIO/GPIO_InfiniteLedToggling_Init/Src/system_stm32f1xx.c      STM32F1xx system source file


@par Hardware and Software environment

  - This example runs on STM32F103xB devices.
    
  - This example has been tested with STM32F103RB-Nucleo board and can be
    easily tailored to any other supported device and development board.


@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
