Back to Release page
# Release Notes for STM32091C_EVAL Applications Copyright 2016 STMicroelectronics
## Update History ### V1.11.0 / 12-September-2019 Main Changes Update for compatibility with FreeRTOS v10.0.1_20190329 Update for compatibility with TouchSensing v2.2.4 Update stm32f0xx_hal_conf.h files : Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Add reference to HAL EXTI driver Add registers callbacks defines ### V1.9.0 / 25-August-2017 Main Changes Maintenance release. Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Align stm32f0xx_hal_conf.h with latest template defined in HAL. Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Update STEMWIN_HelloWord .cproject file to be compliant with Linux platforms. Remove Cortex-M3/M4 specific defines and macros in FreeRTOSConfig.h from all FreeRTOS based applications. ### V1.8.0 / 07-April-2017 Main Changes Maintenance release Update stm32f0xx_hal_conf.h files : Compliance with MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). Add definition of USE_SPI_CRC Update FreeRTOS_Semaphore and FreeRTOS_ThreadCreation examples to be aligned with latest reference code. ### V1.7.0 / 04-November-2016 Main Changes Maintenance release Change in HAL API for TIM : add AutoReloadPreload capability in TIM handler. Impacts in USB Device example and in all FreeRTOS examples. Updated FreeRTOS examples to call TIM HW function as time base source instead of Systick ; changes in examples : FreeRTOS Low Power FreeRTOS Mutexes FreeRTOS_Queues FreeRTOS Semaphore FreeRTOS Thread Creation FreeRTOS Timers Updated STemWin version : STemWin532 “build 20160205” ### V1.6.0 / 27-May-2016 Main Changes Maintenance release. Updated system_stm32f0xx.c files: Added APBPrescTable definition. Updated HEAP size for FreeRTOS applications (updates in FreeRTOSConfig.h). Updated IAP applications following HAL UART modifications. ### V1.5.0 / 29-January-2016 Main Changes Maintenance release. Add support of System Workbench for STM32 (SW4STM32) toolchain. Updated GPIO Output Speed literals naming to ensure HAL full compatibility. Added IAP applications using the USART: IAP/IAP_Main, IAP/IAP_Binary_Template projects. Updated FatFS\FatFS_uSD application: increased size of heap/stack for proper execution. Updated system_stm32f0xx.c files: Removed __IO or __I on constant table declaration. Added HSI48_VALUE definition. Updated stm32f0xx_hal_conf.h files: Set HSE_STARTUP_TIMEOUT value to 100ms instead of 5000ms Updated “Liberty” License with the new license “Ultimate Liberty”. ### V1.3.0 / 26-June-2015 Main Changes Adapt projects to use STemwin V5.28 “ST modified 20150415“ (Changed lib name from 526 to 528). Adapt existing projects to use FreeRTOS V8.2.1. Adding new projects to introduce the FreeRTOS V8.2.1 FreeRTOS_SignalFromISR (thread signaling from an interrupt) FreeRTOS_Signal (thread signaling) FreeRTOS_Mail (mail queues) Fix known defects and several enhancements implementation. Complete HAL API alignment (renaming). ### V1.2.0 / 05-Dec-2014 Main Changes Update for compatibility with: FatFS R0.10b_STM32Cube_20141120 USB_device V2.3.0 FreeRTOS V8.1.2_20141204 STemWin STemWinLibrary526_20141020_CM0 ### V1.1.0 / 03-Oct-2014 Main Changes official release. minor correction (compilation warnings) Applications porting on IAR, KEIL, TRUE STUDIO ### V1.1.0RC2 / 01-Aug-2014 Main Changes First beta release supporting STM32091xC device ## License This software component is licensed by ST under Ultimate Liberty license SLA0044, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/SLA0044 For complete documentation on STM32 Microcontrollers visit www.st.com/STM32