Back to Release page
# Release Notes for STM32F072RB-Nucleo Demonstrations Copyright 2016 STMicroelectronics
## Update History ### V1.11.0 / 12-September-2019 Main Changes Update stm32f0xx_hal_conf.h files : Change assert_failed() prototype to be compliant with MISRA C rule 11.4 Add reference to HAL EXTI driver Add registers callbacks defines ### V1.9.0 / 25-August-2017 Main Changes Maintenance release. Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Align stm32f0xx_hal_conf.h with latest template defined in HAL. Change assert_failed() prototype to be compliant with MISRA C rule 11.4 ### V1.8.0 / 07-April-2017 Main Changes Maintenance release Update stm32f0xx_hal_conf.h files : Compliancy with MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). Add definition of USE_SPI_CRC ### V1.7.0 / 04-November-2016 Main Changes Maintenance release. No update ### V1.6.0 / 27-May-2016 Main Changes Maintenance release. Updated system_stm32f0xx.c files: Added APBPrescTable definition. ### V1.5.0 / 29-January-2016 Main Changes Maintenance release. Add support of System Workbench for STM32 (SW4STM32) toolchain. Update for compatibility and alignment with latest Nucleo and Adafruit Shield BSP Drivers. Updated GPIO Output Speed literals naming to ensure HAL full compatibility. Updated system_stm32f0xx.c files: Removed __IO or __I on constant table declaration. Added HSI48_VALUE definition. Updated stm32f0xx_hal_conf.h files: Set HSE_STARTUP_TIMEOUT value to 100ms instead of 5000ms Updated “Liberty” License with the new license “Ultimate Liberty”. ### V1.3.0 / 26-June-2015 Main Changes Upgrade to use FatFs R0.11. Fix known defects and several enhancements implementation. Complete HAL API alignment (renaming). ### V1.2.0 / 05-Dec-2014 Main Changes Update for compatibility with: FatFS R0.10b_STM32Cube_20141104 minor correction for compilation warning with HAL_SPI ### V1.0.0 / 18-Juin-2014 Main Changes First official release. ## License This software component is licensed by ST under Ultimate Liberty license SLA0044, the “License”; You may not use this component except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/SLA0044 For complete documentation on STM32 Microcontrollers visit www.st.com/STM32