CMSIS-Zone (Preview): /capture element

| CMSIS-Zone (Preview) Version 0.0.1 System Resource Management

- Main Page
- Usage and Description

All Files Pages
/capture element

The capture element can be used to specify linker symbol patterns to be placed into the enclosing memory assignment.

Example

<zones>
<pzone name="App" Dname="ARM32CM4128x" Pname="Cortex-M4">
<assign name="SHARED" as="SRAM" access="rwu">
<capture symbol=".bss.shared"/>
<capture symbol=".data.shared"/>
:
</assign>
:
</pzone>
:
</zones>

Schema Description

Parent Element | Element Chain
--- | ---
assign | /assign element
Attributes | Description | Type | Use
cunit | Pattern selecting the compilation unit(s) to be placed into this assignment. | xs:string | optional
symbol | Pattern selecting the symbols to be placed into this assignment. | xs:string | optional
Child Elements | Description | Type | Occurrence
|  | complexType | 0..*